# **BEST FC300 Inverter Settings and Wirings for EasyRoute CNC Router**

<https://am.co.za/>

P087 = **101** Set this value to reset Inverter Parameter to Factory Default, all below settings are based on default

(Reboot after Reset, then change:)

**P017 = 0.5 Stop Breaking Time, 0.5 seconds**

**P018 = 5 DC Breaking Voltage, 5%**

**P038 = 4 Acceleration Time, 4 seconds**

**P039= 5 Deceleration Time, 5 seconds**

(Those should be on default, unless you want to change each gear frequency)

P021 = 400 Maximum frequency for our spindles is 400MHz

P030 = 0 Multi-speed frequency 0 SOFF

P031 = 100 Multi-speed frequency 1 S1

P032 = 150 Multi-speed frequency 2 S2

P033 = 200 Multi-speed frequency 3 S3

P034 = 250 Multi-speed frequency 4 S4

P035 = 300 Multi-speed frequency 5 S5

P036 = 350 Multi-speed frequency 6 S6

P037 = 400 Multi-speed frequency 7 S7 Speed on Panel

Reboot One More Time After All Parameters Changed.

Shape

Description automatically generated with low confidenceBEST FC300 Manual on CNCU.CO.ZA

Text

Description automatically generated with low confidencePage 18, section “3. 4. Parameter modification method” explained how to change above values.

A picture containing table

Description automatically generatedWiring:

You may need to connect GND to PE/COM if its not ground already.