**2022+ Model FastCOLOUR Printer Default Settings**

|  |  |  |
| --- | --- | --- |
| Setting | **F1-18001800mm Single Head** | **F1-1800D****1800mm Double Head** |
| **Factory Settings** |  |  |
| Station | Lift |
| Wiper | Pop, Lift |
| Printing Width | 195cm | 190cm |
| Raster Type | B |
| Cart Motor | DC | Servo |
| Paper Motor | Step |
| Wiper Direction | Normal |
| Paper Direction | Reverse |
| Car Direction | Cannot Change. If Cart Move Wrong Direction, Swap Wires |
| Acc Distance | 80mm |
| Paper Speed | 50 |
| LCD Type | B |
| UV Type | D |
| Auto Clean | Spit: Printhead Flush Ink OnlyClean: Full Cleaning Sequence |
| Wiper Speed | Between 60 to 70 |
| Station Speed | 84 |
| Do Wipe Speed | 2 |
| Fan in Mode | 可控 (Adjustable in Menu)常开 (Always On) |
| Head Width | 50mm (for XP600 Printhead |
| Dry Set | Dry: For UV Printer, Control LED LampsHeat: For Solvent/Sublimation etc(P.S Still need to adjust wires) |
|  |  |  |
| **Advance Setup** | *(Password Protected)* |
| Voltage Adjust | 560 |
| Voltage Type | S 097f0600 |
| Colour | CYCcMm |
| Colour Dual Seq. |  | KKCCMMYYCCMM |
| Print Empty | Not Print Empty Pass |
| Print more | 0 |
| Spit Switch | Close |
| Spit Dots | 10 |
| Spit Empty Data | 3 |
| Chang config | All Colour |
| White Repeat |  | 1 Pass (Increase Passed for Density) |
|  |  |
| **UV Lamp Control** | Left LED | Both LEDs (Left & Right) |
| R to L On | 1800 |  | 3600 |
| R to L Off | 8000 |  | 8500 |
| L to R On | 3600 |  | 3600 |
| L to R Off | -1800 |  | 0 |
| Distance  | 5200 |  | 9500 |