**2022+ Model FastCOLOUR Printer Default Settings**

|  |  |  |  |
| --- | --- | --- | --- |
| Setting | **F1-1800 1800mm Single Head** | | **F1-1800D**  **1800mm Double Head** |
| **Factory Settings** |  | |  |
| Station | Lift | | |
| Wiper | Pop, Lift | | |
| Printing Width | 195cm | | 190cm |
| Raster Type | B | | |
| Cart Motor | DC | | Servo |
| Paper Motor | Step | | |
| Wiper Direction | Normal | | |
| Paper Direction | Reverse | | |
| Car Direction | Cannot Change. If Cart Move Wrong Direction, Swap Wires | | |
| Acc Distance | 80mm | | |
| Paper Speed | 50 | | |
| LCD Type | B | | |
| UV Type | D | | |
| Auto Clean | Spit: Printhead Flush Ink Only  Clean: Full Cleaning Sequence | | |
| Wiper Speed | Between 60 to 70 | | |
| Station Speed | 84 | | |
| Do Wipe Speed | 2 | | |
| Fan in Mode | 可控 (Adjustable in Menu)  常开 (Always On) | | |
| Head Width | 50mm (for XP600 Printhead | | |
| Dry Set | Dry: For UV Printer, Control LED Lamps  Heat: For Solvent/Sublimation etc  (P.S Still need to adjust wires) | | |
|  |  | |  |
| **Advance Setup** | *(Password Protected)* | | |
| Voltage Adjust | 560 | | |
| Voltage Type | S 097f0600 | | |
| Colour | CYCcMm | | |
| Colour Dual Seq. |  | | KKCCMMYYCCMM |
| Print Empty | Not Print Empty Pass | | |
| Print more | 0 | | |
| Spit Switch | Close | | |
| Spit Dots | 10 | | |
| Spit Empty Data | 3 | | |
| Chang config | All Colour | | |
| White Repeat |  | | 1 Pass (Increase Passed for Density) |
|  |  | | |
| **UV Lamp Control** | Left LED | Both LEDs (Left & Right) | |
| R to L On | 1800 |  | 3600 |
| R to L Off | 8000 |  | 8500 |
| L to R On | 3600 |  | 3600 |
| L to R Off | -1800 |  | 0 |
| Distance | 5200 |  | 9500 |