en-US

# Customize Frame Grabber's Port

The tool can customize the frame grabber's port.

1. Go to C:\Program Files (x86)\MVS\Applications\Win64 on the PC.
2. Find and open the tool for customizing frame grabber's port SerialPortEnum.exe.
3. The names and ports of the connected devices will be displayed on the left. Select the frame grabber to be edited, and the COM will be displayed on Current COM.

   Only the Hikrobot CML frame grabbers will be displayed.

4. Click on the lower right of Virtual Serial Port to choose a COM from the drop-down list.
5. Click Apply.