en-US

# Status of USB3 Vision Camera

The Software provides multiple icons to indicate the status of the USB3 Vision camera. You can do further management according to the status of the cameras.

The following table shows the descriptions of different status.

Table 1 Status Description
Camera Status | Description
--- | ---
| Available and disconnected. You can double-click the camera or select it and click on the control toolbar to connect it to the Software. Once connected, the status changes to .
| Connected.
| USB driver exception. You should reinstall the USB driver.
| Not available. Another software or process on the same PC is accessing the camera.
| The camera is acquiring image data.
| USB driver exception (the USB interface of the PC is USB 2.0 interface). You should reinstall the USB driver.
| Connected (the USB interface of the PC is USB 2.0 interface).
| Available and disconnected (the USB interface of the PC is USB2.0 interface).
| Not available (the USB interface of the PC is USB 2.0 interface). Another software or process on the same PC is accessing the camera.
| The camera is acquiring image data (the USB interface of the PC is USB 2.0 interface).