en-US

# Error Code List

The error codes of the Software and machine vision camera SDK are as the following.

Software Error Code | Machine Vision Camera SDK Error Code | Description
--- | --- | ---
Normal Code Description
0x00000000 | 0x00000000 | Succeeded. No error.
General error codes.
0x90006100 | 0x80000000 | Incorrect or invalid handle.
0x90006101 | 0x80000001 | The function is not supported.
0x90006102 | 0x80000002 | No more cache can be stored.
0x90006103 | 0x80000003 | Function calling order error.
0x90006104 | 0x80000004 | Incorrect parameter.
0x90006105 | 0x80000006 | Applying for resource failed.
0x90006106 | 0x80000007 | No data.
0x90006107 | 0x80000008 | Not prepared, or the running environment has changed.
0x90006108 | 0x80000009 | Versions mismatch.
0x90006109 | 0x8000000A | No enough storage.
0x9000610A | 0x8000000B | Abnormal image. Package missing may cause the abnormality.
0x9000610B | 0x8000000C | Importing DLL dynamically failed.
0x9000610C | 0x8000000D | No cache can be output.
0x9000610D | 0x8000000E | Incorrect file path.
0x900061FF | 0x800000FF | Unknown error.
Error codes of GenI cameras.
0x90006200 | 0x80000100 | General error.
0x90006201 | 0x80000101 | Invalid parameters.
0x90006202 | 0x80000102 | The value exceeds the range.
0x90006203 | 0x80000103 | Incorrect node property.
0x90006204 | 0x80000104 | Running environment error.
0x90006205 | 0x80000105 | Logic error.
0x90006206 | 0x80000106 | Incorrect accessing condition of node.
0x90006207 | 0x80000107 | Timeout.
0x90006208 | 0x80000108 | Conversion exception.
0x900062FF | 0x800001FF | Unknown error of GenICam.
Error codes of GigE_STATUS.
0x90006300 | 0x80000200 | Command not supported by device.
0x90006301 | 0x80000201 | The address to be accessed does not exist.
0x90006302 | 0x80000202 | No data can be written.
0x90006303 | 0x80000203 | No right to access device.
0x90006304 | 0x80000204 | Device is busy, or disconnected from the Software.
0x90006305 | 0x80000205 | Network Package data error.
0x90006306 | 0x80000206 | Network error.
0x90006307 | 0x80000221 | Duplicated device IP.
Error codes of USB_STATUS.
0x90006400 | 0x80000300 | Reading USB error.
0x90006401 | 0x80000301 | Error occurred when writing the USB.
0x90006402 | 0x80000302 | Device exception.
0x90006403 | 0x80000303 | GenICam error.
0x90006404 | 0x80000304 | Insufficient bandwidth.
0x90006405 | 0x80000305 | Drivers mismatch or no driver.
0x900064FF | 0x800003FF | Unknown USB error.
Error codes of upgrade.
0x90006500 | 0x80000400 | Firmware versions mismatch.
0x90006501 | 0x80000401 | Firmware languages mismatch.
0x90006502 | 0x80000402 | Device upgrade conflict. (The device is already being upgraded.)
0x90006503 | 0x80000403 | Internal error occurred in the camera during upgrade.
0x900065FF | 0x800004FF | Unknown error during upgrade.