en-US

# Resend Packet

Packet resending is a mechanism to ensure image quality by resending the lost or damaged packets during image data acquisition. You can set the packet-resending for the Software, including maximum packet resending percent and the timeout period for packet resending.

You can set the Resend Packet switch to on to enable the Software to resending packets, and then configure the following parameters.

Max. Packet Resending Percent (%)

  The maximum percent of packets resent within one frame (default value: 10%). With larger packet resending percent, you can get more complete image data. Conversely, you can get more real-time image data.

Timeout Period(ms)

  The maximum time period (default value: 50 ms) that the Software can wait between two packets that need to be resent (either for the packet is lost or damaged). If the waiting time exceeds the time you set, the Software will not wait for or resend any packet.

  Note:

  - You can set a relatively long timeout period if there are excessive packet losses.

  - You can set the value of Timeout Period from 0 ms to 1000 ms.

Figure 1 Packet Resending Settings