en-US

# Status of GigE Vision Camera

The Software provides multiple icons to represent different status of GigE Vision cameras.

The following table shows the descriptions of the status of the GigE Vision camera on the device list.

Table 1 Status Description
Camera Status | Description
--- | ---
| Available and disconnected. Note: You can double-click the camera or select it and click on the control toolbar to connect it to the Software. Once connected, changes to .
| Not available. Another Software or process is accessing the camera.
| The camera is on the same subnet with the PC on which the Software runs, but NOT in the same network segment. You should configure its IP address to the same network segment before you can connect and use the camera. Note: You can double-click the camera or click Tool > IP Configurator to configure the camera's IP address. See IP Configurator for details about how to configure camera IP address.
| Connected.
| The camera is acquiring streams. Note: See Acquisition and Live View for details about how to start acquisition.
| Multicast of the camera is enabled on another Software. And the camera is connected to the current Software. Note: See Multicast Settings for details about how to enable Multicast.
| Multicast of the camera is enabled on another Software. And the camera is not connected to the current Software. Note: See Multicast Settings for details about how to enable Multicast.