en-US

# Dead Pixel Correction

You can conduct dead pixel correction on a camera to fix dead pixel.

Make sure that the camera has been connected to the Client.

1. Select a camera on the device list.
2. Right-click the camera name and select Dead Pixel Correction.
3. Optional: Export the dead pixel file and edit the dead pixel information.
4. Select a dead pixel file (MFA format) and click Import.

   A progress bar will be displayed when importing, and a message box noting "Imported" will pop up when the import is finished.