en-US

# Tool

The Software provides multiple tools for camera configuration and management.

The following table shows the brief description of each tool.

Table 1 Tool Description
Tool | Description
--- | ---
IP Configurator | Configure the IP address of the GigE Vision cameras. See IP Configurator for details.
Firmware Updater | Update the firmware of GigE Vision cameras and USB3 Vision cameras. See Firmware Updater.
Import/Export Features | Export the selected cameras' feature configuration information as a MFS file to the local PC, or import the MFS file containing camera feature information from the local PC to the selected cameras. See Import/Export Features of Multiple Devices for details.
Log Viewer | View SDK logs. See Log Viewer Tool for details.
Virtual Camera | Virtual Camera is a tool designed for scenarios where constructing a real setup of camera environment is not feasible. It can simulate cameras and help to simplify tests during development stage.
Bandwidth Manager | Adjust the bandwidth of the connected cameras to avoid excessive packet losses. See Bandwidth Manager for details.
GigE Vision Action Command | Trigger actions in multiple cameras at the same time. See GigE Vision Action Command for details.
Export All Devices Information | Export information of all cameras enumerated on the Software and the information of the current PC in a folder. The information includes device logs, NIC information of the current PC, computer and system information, driver status of the current PC, and camera parameters. The information will be saved as TXT documents.