en-US

# View Acquisition Status

During acquisition or live view, you can view the acquisition status of the camera(s), including the acquisition rate, image number, bandwidth, resolution, errors, packets lost and display rate, etc.

## View Acquisition Status in 1-Window Mode

During acquisition or live view (in 1-Window mode), a status bar appears at the bottom of the display window to display in real time the acquisition status of the selected camera.

You can click in the lower-left corner to select status parameters (the selected ones will be displayed on the status bar).

For GigE Vision cameras, you can select the following status parameters: acquisition rate, image number, bandwidth, resolution, errors, packet lost, packets requested to resend, packets resent, display rate, location, RGB, YUV, zoom, and temperature.

Figure 1 GigE Vision Camera Acquisition Status

For USB3 Vision cameras, you can select the following status parameters: acquisition rate, image number, bandwidth, resolution, errors, packet lost, display rate, location, RGB, YUV, zoom, and temperature.

Figure 2 USB3 Vision Camera Acquisition Status

## View Acquisition Status of Multiple Cameras Simultaneously

During live view of multiple cameras, you can click to open the Status window to view the acquisition status of these cameras. After that, you can click More to open the parameter panel, and then select parameters to be displayed on the Status window or status bar.

Figure 3 The Status Window