en-US

# Configure Grid

You can configure grids on the image when acquiring image data in 1-window mode. This is especially helpful when you need to align objects on the image.

1. Connect a camera and then start acquisition in 1-window mode.
   Note:

   For details about image acquisition in 1-window mode, see Acquisition and Live View in 1-Window Mode.

2. Click to display grids on the image.
   Figure 1 Grids Displayed on Image
3. Optional: Click (beside ) to configure grid parameters, including grid spacing and color.
   Grid Spacing

     Set the grid spacing value. You can set the value to 30, 60, or 90. You can also customize a value as required. The larger the value, the more scattered the grids will be.