en-US

# ISP

Follow the instructions below to configure the ISP parameters.

Gamma Enable

  Enable the gamma correction of pixel intensity, which helps optimizing the brightness of acquired images for displaying on a monitor.

Gamma Selector

  Specify a gamma correction mode.

  User

    The gamma correction value can be entered manually for the Gamma parameter as desired.

  sRGB

    The gamma correction value will be automatically set to approximately 0.4. This value is optimized for image display on sRGB monitors.

Gamma

  The gamma correction value.

Sharpness Enable

  If enabled, the Sharpness parameter will be available. The larger the Sharpness value, the more distinct the contours of the image objects will be. This is especially useful in applications where cameras must correctly identify numbers, letters or characters.

Hue Enable

  Enables/disables hue adjustment.

Hue

  Hue of the image in degrees.

Saturation Enable

  Enables/disables saturation adjustment.

Saturation

  Saturation of the image in percent.

Balance White Auto

  Balance White Auto is the 'automatic' counterpart of the manual white balance feature.

Bayer Interpolation Method

  If you select Bayer as the pixel format, select Quick, Balance, or Optimal as the bayer interpolation method.