en-US

# Import/Export Features of Multiple Devices

On Import/Export Features window, all the GigE Vision cameras on the same local subnet with the PC on which the Software runs, the connected USB3 Vision camera, the connected Camera Link cameras will be displayed automatically. You can select camera(s) and then export their feature configurations to the local PC as MFS files, or import MFS files to fast load the feature configurations to the camera(s).

Note:

The Software does not support importing or exporting features of multiple frame grabbers.

1. Open the Import/Export Features window in one of the following two ways.

   - Click Tool > Import/Export Features.

   - Click Import_Export_Features in the installation directory of the Software.

   Figure 1 Import/Export Feature Window
2. Optional: Click to select the to-be-displayed information (model name, device user ID, MAC address, etc.).
3. Select an interface from the interface list on the left.
4. Select cameras under the selected interface.
   Note:

   - Up to 20 cameras can be selected.

   - You can only select the cameras of Free status.

5. Export or import the features of the selected cameras.

   - Click Export to export the features of the selected cameras as a MFS file.

     Note:

     The exported MFS file is named as "camera model_serial number" by default and the name cannot be edited by default. Example: MV-CA060-11GM_00604207150.

   - Click Import to select a MFS file so as to import the features saved in the file to the selected cameras.

     Note:

     - The progress and results of the operation are displayed on the Operation Status column.

     - You can view the exception information and error code if importing features to a specific camera fails.