en-US

# Configure White Balance (YUV/RGB/BGR)

If the Pixel Format parameter of the camera is set to YUV, RGB or BGR, you can go to the White Balance section of the Common Features tab to set the white balance parameters.

Note:

- White balance parameters in only available for color camera.

- The available parameters vary with different camera models.

Balance White Auto

  Set the mode for automatic white balancing between the color channels. Once set, the white balancing ratios are automatically adjusted.

  Off

    Set white balancing manually using Balance Ratio Selector and Balance Ratio.

  Once

    White balancing is automatically adjusted once by the camera. Once it has converged, it automatically returns to the Off state.

  Continuous

    White balancing is constantly automatically adjusted by the camera.

Balance Ratio Selector

  Selects which Balance ratio to control.

  Red

    Balance Ratio will be applied to the red channel.

  Green

    Balance Ratio will be applied to the green channel.

  Blue

    Balance Ratio will be applied to the blue channel.

Balance Ratio

  Set the weight value (0 to 4095) for the channel selected from Balance Ratio Selector.