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	You can edit Chinese, number, English, symbols, and so on.
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	Delete the information segment that has been edited
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	Edit variable in year, month, day, hour, minute and second.
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	Create a new information segment.
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	Editable variable serial number, regular number
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	select the name of the information that has been saved
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	Click Run to star printing or stop printing.
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	Click to save the message name,

Long press for more than 5 seconds to save as
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	Edit the trade mark or logo.
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	Reedit the information name
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	Edited Barcode、form、

TXT、Excel、Segmented
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	Minute movement of information segment position
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	System parameters can be set (under the guidance of the engineer)
	Production
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	Percentage of battery usage (general reference only)）
	Information
	Currently printable information name
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	Click to enlarge once, and long press to enlarge continuously
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	Click zoom out once, and long press continue to zoom out
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	Turn 0、90、180、270、360 degree
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	Printing parameter settings (under the guidance of engineers)
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Printer packing list

	NO
	Part name
	Qty
	Exterior
	Handheld
	Online

	1
	Packing Box
	1
	
	★
	★

	2
	Hand held Ink jet Printer
	1
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	★
	

	3
	Online Ink Jet Printer
	1
	
	
	★

	4
	Charger

(16.8V 1A)
	1
	
	★
	

	5
	Adapter

(16V-3A)
	1
	
	
	★

	6
	Sensor
	1
	
	
	★

	7
	Ink cartridge
	1
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	〇
	〇

	8
	Stylus
	1
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	★
	★

	9
	Printer operation manual
	1
	
	★
	★



        




技术参数

	Machine size 
	140*53*238mm（Include handle）

	Material of Printer Outside
	ABS outside

	Weight
	约800g（without ink cartridge）

	Screen size
	5 inchs touch screen（108*65mm ) \ 800*480dpi

	Store information
	Infinite storage

	Precision of printing
	300DPI/600DPI(half only)

	Counting unit
	1-15digits

	Printing bar code
	Bar code, QR code, variable QR code

	External interface
	Charging interface, R232 serial port, USB

	Using environment
	Temper:0-40℃、humidity:10-80%

	Oil ink color 
	Black, red, blue, green, yellow, orange, white, invisible

	Fast dry ink color 
	Black, red, blue, green, yellow, orange, white, invisible

	 Ink cartridge capacity
	42CC（1/2 inch）、45CC（1 inch）

	Ink type
	Dry, oily, water-based

	Spray print library
	Synchronize with machines and computers

	Spray printing distance
	2-5mm

	printing height
	2-12.7mm、2-25.4mm、2-48mm

	Speed of printing
	60m/min

	Printing content
	Date, counting, batch number, serial number, pictures etc

	Power parameters
	DC 14.8V lithium battery;

16V3A/5A the power adapter

	Battery capacity
	1500-2600mAh


English version





Touch





Please read the instruction manual carefully before using and keep it properly.


The picture related to this manual for reference only. All contents are checked and proofread. If there are any problems such as printing errors, please understand





A series general-purpose for Touch


The operation manual of


the GoPrinter








Intelligent Ink Jet Printer








Disclaimer：


1.During the use of this product, if there is serous damage, accidental fire, water ingress, unexplained chemical corrosion, unauthorized dis assembly, etc, it isn’t covered by the warranty.


2.If the printer has malfunctioned, please back up the information in time to prevent loss before repairs.


3.If the use of the code jet machine is abnormal, please contact the maintenance engineer or call the manufacturer’s service line.


4.Untrained personnel are strictly prohibited to operate and use the jet printer


5.It is strictly prohibited to disassemble the printer without the permission of the factory staff.


6.The operator of the ink-jet machine should read the instruction carefully before operating the machine.


7.The company reserves the right to interpret this disclaimer.





Precautions for use of


quick-drying ink cartridges





1.The power supply of the machine must be cut off before loading and unloading the ink cartridge


2.If you do not use the machine for more than 20 minutes, you must remove the cartridge from the machine. And clip it with the card.(Be sure to save the clip)


3.Specific requirements based on the nature of the ink cartridge, you are better to use ink cartridge out  after opening ink cartridge.


4.Because the cartridge is quick dry nature, so the use of the process of a little drawing, missing line phenomenon, is a normal situation


5. If there is a phenomenon of a little drawing or missing line , you can use a soft paper towel to wipe the nozzle in one direction (Do not damage the nozzle with hard materials)


6.If it is fast dry white ink, shake it for 5-10 minutes before each use, otherwise the color will be lighter.(Be careful not to shake too hard）





0.5inch ink cartridg（12.7mm）





1inch ink cartridge（25.4mm）











Half inch 


handheldHandle


 to the rear





One inch 


metal case


 for handheld





Half inch


metal case


for handheld











Special modified type





Touch-D(Double head)





Handheld jet printer Positive


The handle (inside the battery) 


Print switch


Auxiliary wheel               


Nozzle slot     


Edit unction area         


Display area 





Handheld jet printer other side


7、R232 serial port       


8、Auxiliary wheel  


9、USB serial port       


10、Charging interface(17V)  


11、Synchronizer        


12、Transmission belt 


13、Power switch








（T-Y main menu）





（T-D main menu）





（T-X main menu）





Click on the power switch


And turn on the boot page


（The boot time is abut 7 seconds）





Boot interface











1.TEXT








   Handwriting input interface





Handwritten location：Handwritten text area


Selected location ：Choose the correct text


Delete：Clear handwriting Location’s text


<-------：Clear confirmed area text





   Click"text"Enter the above interface，where you can edit Chinese、English、number、symbol and so on








Insert date





Insert counter





Turn page selection





Switch input method





Delete characters





Click font settings





Font: Song Ti, Kai Ti, Li Shu, Hei, etc.


Style: entity font, dot matrix font, deleted  font


Text  height: 0-500


Text  width: 0-999


Text  interval: 0-99


Rotation  angle: 0-360 degree single  font  rotation


Note the difference with 


overall rotation unction


Font style: regular, bold, italic, bold italic





Touch-X:The highest printing height is 12.7mm


Touch-Y:The highest printing height is 25.4mm


Touch-D:The highest printing height is 48mm








Click "Date", and select the


corresponding date or time format.


Validity period: set year, month and day


(Used in combination with production date)


Font setting: see "Page 7" for details





2.Date








 Validity period setting





Half-width symbol


Full-width symbols cause character spacing to increase





Full-width symbol





  Commonly used pictures





3.Picture





Common icons: R mark, diameter mark, handle with care, disable hand hook, etc. The printer system comes with it.


    U Disk: Read the picture in the U disk and import it into the printer. It must be in BMP format, which can recognize pictures in Chinese and English and character names (only monochrome bitmaps).





Do not pull out the USB flash drive during the printing process, otherwise the file will be missing and the warning shown in the above picture will appear.





After the USB flash drive reads the file, select the picture to be printed and import it, and the width and height of the picture can be can be adjusted by yourself. 


The recommended size is 145 pixels for a half-inch picture, 290 pixels for a one-inch picture, and 580 pixels for a double-headed picture


   Reverse: the black part becomes white, and the white part becomes black.


   Rotation Angle: Support 360 degree rotation.





Entry system: decimal, hexadecimal


Number of repetitions: the number of repeated printing


Number of digits: counting digits (1-15 digits)


Step: the step size of the count change


Change: self-increasing, self-decreasing


Maximum value: the end value of the count


Current value: the current value of the count


Minimum: the start value of the count


Font setting: see "page 7" for details


Leading zero: yes (such as 0001, 0002, 0003), no (such as 1, 2, 3)





  More: barcode, Table, TXT file, Excel , Paragraph,Remote data.





5.More








4.Counter








Table: A blank table with 4 rows and 5 columns can be inserted at most, and the thickness of the lines can be adjusted


Row height: 10-150


Column width: 10-999


Merge cells: support





  Barcode type: ENA13, CODE128, QR code, DM code, etc.


    Transverse stretching: freely modify the value to change the width and width ratio of the two-dimensional code to ensure that the two-dimensional code printed out is square.


    When printing barcode, you can choose whether to display barcode text and barcode text size.


   Gs1 barcode editing instructions: The text content must be entered in the half corner state. The input content must be accurate or the graphic code cannot be generated.





Barcode: Enter the text to be recognized in the right box, and the corresponding bar code will be displayed in the left box.


Graphic code setting: change the bar code type





 TXT file: Read the U Flash drive information, select the corresponding txt file and click "Import".


    Import TXT files by searching for file names





  The right area will preview the content of the txt file, slide up in the blank area to preview the content below, the bottom right corner displays the total number of lines; 


   Character interception: can be arbitrary interception character printing；


  Start line: select which line to start printing from;


  Repeat:each message is printed repeatedly;


  Font setting: see "Page 7" for details;


  Generate barcode: After checking, the upper left corner becomes select code ". After selecting the corresponding barcode type, the printer will automatically generate and print the corresponding barcode according to the txt information. See "Page 10" for details





   The right area will preview the content of the excel file, slide up in the blank area to preview the content below, the bottom right corner displays the total number of rows;


  Column: Select a column to preview the information of the corresponding column;


Start line: select which line to start printing from;


  Character interception: can be arbitrary interception character printing；


  Start line: select which line to start printing from;


  Repeat: each message is printed repeatedly;


  Font setting: see "Page 7" for details;


  Generate barcode: After checking, the upper left corner will become "select code setting". After selecting the corresponding barcode type, the printer will automatically generate and print the corresponding barcode according to the information in the excel form. See "Page 10" for details.





   EXCEL file: read the U disk information, select the corresponding EXCEL file and click "Import". (Only for files in .xls format)


    Import Excel files by searching for file names





Record import and export


Record import: import printing information from u disk.


Record export: export the printing information to a USB flash drive.


The imported file is shown in the figure below.





Click "Segment" to realize segment printing. A segment symbol will appear in the main edit box.





6.setting








Photoelectric encoder detection


Photoelectric signal: Use with photoelectric sensor, display "ON" when sensing, and "OFF" when not sensing


Encoder: Display the number of pulses received.





Time setting


 Set the calendar: Gregorian calendar, Persian calendar, Islamic calendarSet the system time, including year, month, day, hour, minute, and second.





Language selection


Simplified Chinese, Traditional Chinese, English, Russian, Japanese, German, French, Korean, Italian, Polish, Dutch, Finnish, Arabic, Danish, Czech, Swedish, Vietnamese, Greek, Turkish , Spanish, Portuguese, Persian, Thai





information


   Check update: Update the system version. Contact Huawei technical support.


  Manufacturer information: Change the name at the upper left corner of the main page. The character cannot be too long.


   Output clearing: clear total output data


   Factory mode: Contact factory engineers.


   Software: Displays the current  software version.


    About: Hardware information





7.Printing setting








Print direction


Upside: printing information from right to left


Reverse: Print the information vertically





Setting


  Key tone: On, off


  Restore:Clear all information and parameters


   Screen off: used to adjust when the touch screen is inaccurate Automatic breath screen: Free to set the screen saver time


.





Nozzle set


   L or R: left nozzle, right nozzle, simultaneous printing (only half inch model)Left and right spacing: for simultaneous printing, the left and right spacing can be adjustedLeft side and right side overlap (only half inch model)


   Voltage: 8.6-9.2V recommended for quick-drying cartridgesWater-based cartridges are recommended at 10.5-11.5VFor special cartridge types, consult the manufacturer's engineer


   Pulse width:1.6-2.2μsFor special cartridge types, consult the manufacturer's engineer


  Jet times: normal, bold 1-9 times, recommended to use the normal option, bold will increase the amount of ink consumption.





Synchronously


   Encoder switch: on, off


   Encoder div: the larger the value, the wider the number of prints and the longer the information


   Speed: the larger the value, the faster the ink output speed, the maximum value is 50000


   Frequency doubling: the larger the value, the longer the printed characters, but the number of printed columns will not change.





 Continuous print control


  Off: The automatic printing function is turned off. You can only print with the handle button.


  Timing: Automatically print a message at regular intervals. The interval time is set from the continuous print interval. And turn off the encoder.


  Encoder: A message is automatically printed every certain pulse number, and the interval pulse number is set by the continuous printing interval.


   Continuous printing Settings:First, when set to "timing", according to the set time and times, click "after start printing" code jet printer will immediately print.2. When set as "encoder", according to the set interval and times, it is necessary to move the code jet printer for printing after clicking "start printing".





Photoelectricity: ON、OFF


  Sensor phase: For details, please contact after-sales engineers


  Continuous printing times: the corresponding number of photoelectric induction for one spray


  Printing interval: the larger the value, the larger the interval


  Delay: After triggering printing, printing for an extended period of time(When the encoder is started, the pulse signal of the encoder is collected by default for printing)


  Photoelectric signal unit: millisecond pulse signal unit: point





Print head setting (for T-D inkjet printer)


 Nozzle selection:


Nozzle 1 (No. 1 nozzle is used alone)


Nozzle 2 (No. 2 nozzle is used alone)


Double nozzle splicing (splicing nozzles 1 and 2)


  Overlap: ensure that the nozzles 1 and 2 are aligned in the horizontal direction


  Printer spacing: ensure that nozzles 1 and 2 are aligned in the vertical direction


If the synchronization frequency multiplication and encoder frequency division are changed, the above two parameters need to be re-adjusted


    The voltage value and pulse width value should be carefully adjusted according to the ink cartridge type under the guidance of the manufacturer's engineer! ! ! To avoid the risk of damaging the machine and ink cartridges.





Other settings


   Print sound: off, only start, only finish, start & finish, automatic (manual printing mode start and end will have sound prompt, sensor printing only start printing with sound prompt, end printing without prompt), turn off the printing sound can improve the printing speed to a certain extent


   Screen refresh: Update the screen display when printing


  Gap free printing: print the same content continuously


   Print times: Number indicates times (please do not change)


   Spray setting: The value represents milliseconds


   High DPI: enable 300dpi. Shut down 150 dpi


   Real printing time: Real-time printing time refresh.





The validity period is user-defined


After clicking "YY", the following interface will appear.


1. Click Validity Period to customize the setting format.


2. Replace the year, month, day, and day with special characters.


3. It automatically displays the current day of the year.





Touch Series DB9 pin wiring diagram





Note: It is recommended to use floor stand for online inkjet printers!


Note:“★”to be standard,“〇”pay for








 The series of Touch Printer Size chart








140mm





Fixed bracket with online machine installation diagram








Physical picture of fixed bracket


 (including Sensor)








(T-XY)





(T-D)





120mm





140mm





98mm





53mm





140mm





80mm





235mm





90mm





50mm





Note: the above common accessories need extra payment








Conveyor belt 





Floor stand 





Printing Board








printing platform








Commonly used accessories For 


The Series of Touch Printer








These parameters are subject to change without prior notice













