**Error E1: Short Circuit Error**

* If errors persist without connecting any attachment, the **Control Unit** has Short Circuit, and needs to be replaced.
* If error E1 after connecting an attachment, cause might be:
  + Heating element short circuit (need to replace)
  + Wrong wiring, might be temperature sensor presented (likely, if not our attachment)

**Error E2: Open Circuit Error**

* No attachment connected, connect an attachment.
* If an attachment connected, causes might be:
  + the heating element inside might be burnt (check continuity to make sure)
  + Wrong wiring, no close loop present (likely, if not our attachment)

**Error E3: Thermal Sensor Init Error**

The **Control Unit** damaged, needs to be replaced.

----------------------------------

**SKU for Spare Parts:**

|  |  |
| --- | --- |
| **H-CONTROL** | Heatware Heat Press **Control Unit** with Temperature & Timer Controller |
| **H-PRESS/CAP** | Heatware Heat Press Caps, Hats & Beanies Heating Pad |
| **H-PRESS/CUP350** | Heat Press 350ml Cone Shaped Cups Heading Pad Attachment |
| **H-PRESS/CUP500** | Heat Press 500ml Cone Shaped Cups Heading Pad Attachment |
| **H-PRESS/DISK12** | Heatware Heat Press Φ120mm+ Round Disk Heating Pad |
| **H-PRESS/DISK15** | Heatware Heat Press Φ150mm+ Round Disk Heating Pad |
| **H-PRESS/FLAT** | Heatware Heat Press 290×380mm Flat Heating Board Attachment |
| **H-PRESS/FLAT/E** | Heatware Heat Press 380×380mm Flat Heating Board Attachment |
| **H-PRESS/MUG240** | Heatware Heat Press 240ml Cylinder Mugs Heading Pad Attachment |
| **H-PRESS/MUG320** | Heatware Heat Press 320ml Cylinder Mugs Heading Pad Attachment, with Connector |

|  |  |
| --- | --- |
| **H-MAT/2938** | Silicone Foam Rubber Mat, 290×380mm Size and 8mm Thickness (Blue) |
| **H-MAT/3838** | Silicone Foam Rubber Mat, 380×380mm Size and 10mm Thickness (Brown) |
| **H-PRESS/ARM** | Heatware Multitalent Heat Press Extension Arm with Column Housing |
| **H-PRESS/ARM/E** | Heatware Multitalent Heat Press Extension Arm with Column Housing for 3838 Heat Press Unit |
| **H-PRESS/CUP** | Heatware Heat Press Cup and Mug Press and Lock Stand |
| **H-PRESS/HANDLE** | Heatware Multitalent Heat Press Handwheel with Crank Handle, Shank 10mm, Diameter 80mm |