云模块版本:2.1.0.0
DATA SUBCRIBER:[CLOUD_PLATFORM,]
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
server-addr:http://pt.hosonsoft.com:5000/footstone-server/api/kdata
HTTP丢包率：0/0
data[type=512,serial=006EA1B2C3D4E5202412170957280000] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_800, M_800, L_800, [FLASH]S_800, M_800, L_800
Total consumption of ink on startup：1_[C], [PRINT]S_800, M_800, L_800, [FLASH]S_800, M_800, L_800
Total consumption of ink on startup：2_[M], [PRINT]S_800, M_800, L_800, [FLASH]S_800, M_800, L_800
Total consumption of ink on startup：3_[Y], [PRINT]S_800, M_800, L_800, [FLASH]S_800, M_800, L_800
Total consumption of ink on startup：8_[W], [PRINT]S_3200, M_3200, L_3200, [FLASH]S_3200, M_3200, L_3200
Total consumption of ink on startup：9_[V], [PRINT]S_3200, M_3200, L_3200, [FLASH]S_3200, M_3200, L_3200
iot_ccid:CCID-123, imei:IMEI-123
push data[type=512, serial=MBCP00000001, len=386] via MB SUCCESSED, 剩余:0
data[type=256,serial=006EA1B2C3D4E5202412170957290001] 入待发送队列
data[type=128,serial=006EA1B2C3D4E5202412170957290002] 入待发送队列
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202412170957280000,提交成功(0)
push data[type=128, serial=MBCP00000002, len=404] via MB SUCCESSED, 剩余:1
iot_status:0
RECV data from IOT, len=532
iot基站数据(serial:0000000000, 流水:006EA1B2C3D4E5202412170957290002,提交成功(0)
push data[type=256, serial=MBCP00000003, len=468] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
iot-sim数据(serial:0000000000, 流水:006EA1B2C3D4E5202412170957290001,提交成功(0)
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
Total consumption of ink on startup：0_[K], [PRINT]S_1200, M_1200, L_1200, [FLASH]S_1040, M_1040, L_1040
Total consumption of ink on startup：1_[C], [PRINT]S_1200, M_1200, L_1200, [FLASH]S_1040, M_1040, L_1040
Total consumption of ink on startup：2_[M], [PRINT]S_1200, M_1200, L_1200, [FLASH]S_1040, M_1040, L_1040
Total consumption of ink on startup：3_[Y], [PRINT]S_1200, M_1200, L_1200, [FLASH]S_1040, M_1040, L_1040
Total consumption of ink on startup：8_[W], [PRINT]S_4800, M_4800, L_4800, [FLASH]S_4160, M_4160, L_4160
Total consumption of ink on startup：9_[V], [PRINT]S_4800, M_4800, L_4800, [FLASH]S_4160, M_4160, L_4160
HTTP丢包率：0/3
data[type=512,serial=006EA1B2C3D4E5202412170958290003] 入待发送队列
push data[type=512, serial=MBCP00000004, len=396] via MB FAILED, 剩余:0
iot_status:0
RECV data from IOT, len=532
HTTP丢包率：0/3
data[type=512,serial=006EA1B2C3D4E5202412170959300004] 入待发送队列
push data[type=512, serial=MBCP00000005, len=396] via MB FAILED, 剩余:0
iot_status:0
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
Total consumption of ink on startup：0_[K], [PRINT]S_1600, M_1600, L_1600, [FLASH]S_1080, M_1080, L_1080
Total consumption of ink on startup：1_[C], [PRINT]S_1600, M_1600, L_1600, [FLASH]S_1080, M_1080, L_1080
Total consumption of ink on startup：2_[M], [PRINT]S_1600, M_1600, L_1600, [FLASH]S_1080, M_1080, L_1080
Total consumption of ink on startup：3_[Y], [PRINT]S_1600, M_1600, L_1600, [FLASH]S_1080, M_1080, L_1080
Total consumption of ink on startup：8_[W], [PRINT]S_6400, M_6400, L_6400, [FLASH]S_4320, M_4320, L_4320
Total consumption of ink on startup：9_[V], [PRINT]S_6400, M_6400, L_6400, [FLASH]S_4320, M_4320, L_4320
RECV data from IOT, len=532
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=2,serial=006EA1B2C3D4E5202412170959550005] 入待发送队列
push data[type=2, serial=MBCP00000006, len=1019] via MB SUCCESSED, 剩余:0
iot_status:0
RECV data from IOT, len=532
作业数据(serial:0000000000, 流水:006EA1B2C3D4E5202412170959550005,提交成功(0)
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
Total consumption of ink on startup：0_[K], [PRINT]S_2000, M_2000, L_2000, [FLASH]S_1320, M_1320, L_1320
Total consumption of ink on startup：1_[C], [PRINT]S_2000, M_2000, L_2000, [FLASH]S_1320, M_1320, L_1320
Total consumption of ink on startup：2_[M], [PRINT]S_2000, M_2000, L_2000, [FLASH]S_1320, M_1320, L_1320
Total consumption of ink on startup：3_[Y], [PRINT]S_2000, M_2000, L_2000, [FLASH]S_1320, M_1320, L_1320
Total consumption of ink on startup：8_[W], [PRINT]S_8000, M_8000, L_8000, [FLASH]S_5280, M_5280, L_5280
Total consumption of ink on startup：9_[V], [PRINT]S_8000, M_8000, L_8000, [FLASH]S_5280, M_5280, L_5280
HTTP丢包率：0/4
data[type=512,serial=006EA1B2C3D4E5202412171000310006] 入待发送队列
push data[type=512, serial=MBCP00000007, len=396] via MB FAILED, 剩余:0
HTTP丢包率：0/4
data[type=512,serial=006EA1B2C3D4E5202412171001320007] 入待发送队列
push data[type=512, serial=MBCP00000008, len=396] via MB FAILED, 剩余:0
HTTP丢包率：0/4
data[type=512,serial=006EA1B2C3D4E5202412171002330008] 入待发送队列
push data[type=512, serial=MBCP00000009, len=396] via MB FAILED, 剩余:0
HTTP丢包率：0/4
data[type=512,serial=006EA1B2C3D4E5202412171003340009] 入待发送队列
push data[type=512, serial=MBCP00000010, len=396] via MB FAILED, 剩余:0
HTTP丢包率：0/4
data[type=512,serial=006EA1B2C3D4E5202412171004350010] 入待发送队列
push data[type=512, serial=MBCP00000011, len=396] via MB FAILED, 剩余:0
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=1,serial=006EA1B2C3D4E5202412171005100011] 入待发送队列
push data[type=1, serial=MBCP00000012, len=978] via MB FAILED, 剩余:0
HTTP丢包率：0/4
data[type=512,serial=006EA1B2C3D4E5202412171005360012] 入待发送队列
push data[type=512, serial=MBCP00000013, len=396] via MB FAILED, 剩余:0
HTTP丢包率：0/4
data[type=512,serial=006EA1B2C3D4E5202412171006370013] 入待发送队列
push data[type=512, serial=MBCP00000014, len=396] via MB FAILED, 剩余:0
HTTP丢包率：0/4
data[type=512,serial=006EA1B2C3D4E5202412171007380014] 入待发送队列
push data[type=512, serial=MBCP00000015, len=396] via MB FAILED, 剩余:0
HTTP丢包率：0/4
data[type=512,serial=006EA1B2C3D4E5202412171008390015] 入待发送队列
push data[type=512, serial=MBCP00000016, len=396] via MB FAILED, 剩余:0
HTTP丢包率：0/4
data[type=512,serial=006EA1B2C3D4E5202412171009400016] 入待发送队列
push data[type=512, serial=MBCP00000017, len=396] via MB FAILED, 剩余:0
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=1,serial=006EA1B2C3D4E5202412171010100017] 入待发送队列
push data[type=1, serial=MBCP00000018, len=978] via MB FAILED, 剩余:0
HTTP丢包率：0/4
data[type=512,serial=006EA1B2C3D4E5202412171010410018] 入待发送队列
push data[type=512, serial=MBCP00000019, len=396] via MB FAILED, 剩余:0
iot_status:0
RECV data from IOT, len=532
HTTP丢包率：0/4
data[type=512,serial=006EA1B2C3D4E5202412171011420019] 入待发送队列
push data[type=512, serial=MBCP00000020, len=396] via MB SUCCESSED, 剩余:0
Total consumption of ink on startup：0_[K], [PRINT]S_2400, M_2400, L_2400, [FLASH]S_1360, M_1360, L_1360
Total consumption of ink on startup：1_[C], [PRINT]S_2400, M_2400, L_2400, [FLASH]S_1360, M_1360, L_1360
Total consumption of ink on startup：2_[M], [PRINT]S_2400, M_2400, L_2400, [FLASH]S_1360, M_1360, L_1360
Total consumption of ink on startup：3_[Y], [PRINT]S_2400, M_2400, L_2400, [FLASH]S_1360, M_1360, L_1360
Total consumption of ink on startup：8_[W], [PRINT]S_9600, M_9600, L_9600, [FLASH]S_5440, M_5440, L_5440
Total consumption of ink on startup：9_[V], [PRINT]S_9600, M_9600, L_9600, [FLASH]S_5440, M_5440, L_5440
iot_status:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202412171011420019,提交成功(0)
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=2,serial=006EA1B2C3D4E5202412171011420020] 入待发送队列
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=1,serial=006EA1B2C3D4E5202412171011420021] 入待发送队列
push data[type=1, serial=MBCP00000021, len=1018] via MB SUCCESSED, 剩余:1
RECV data from IOT, len=532
作业数据(serial:0000000000, 流水:006EA1B2C3D4E5202412171011420021,提交成功(0)
push data[type=2, serial=MBCP00000022, len=1018] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
作业数据(serial:0000000000, 流水:006EA1B2C3D4E5202412171011420020,提交成功(0)
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
HTTP丢包率：0/7
data[type=512,serial=006EA1B2C3D4E5202412171012430022] 入待发送队列
RECV data from IOT, len=532
push data[type=512, serial=MBCP00000023, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202412171012430022,提交成功(0)
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
Total consumption of ink on startup：0_[K], [PRINT]S_2800, M_2800, L_2800, [FLASH]S_1600, M_1600, L_1600
Total consumption of ink on startup：1_[C], [PRINT]S_2800, M_2800, L_2800, [FLASH]S_1600, M_1600, L_1600
Total consumption of ink on startup：2_[M], [PRINT]S_2800, M_2800, L_2800, [FLASH]S_1600, M_1600, L_1600
Total consumption of ink on startup：3_[Y], [PRINT]S_2800, M_2800, L_2800, [FLASH]S_1600, M_1600, L_1600
Total consumption of ink on startup：8_[W], [PRINT]S_11200, M_11200, L_11200, [FLASH]S_6400, M_6400, L_6400
Total consumption of ink on startup：9_[V], [PRINT]S_11200, M_11200, L_11200, [FLASH]S_6400, M_6400, L_6400
iot_status:0
RECV data from IOT, len=532
HTTP丢包率：0/8
data[type=512,serial=006EA1B2C3D4E5202412171013440023] 入待发送队列
push data[type=512, serial=MBCP00000024, len=396] via MB FAILED, 剩余:0
HTTP丢包率：0/8
data[type=512,serial=006EA1B2C3D4E5202412171014450024] 入待发送队列
push data[type=512, serial=MBCP00000025, len=396] via MB FAILED, 剩余:0
HTTP丢包率：0/8
data[type=512,serial=006EA1B2C3D4E5202412171015460025] 入待发送队列
push data[type=512, serial=MBCP00000026, len=396] via MB FAILED, 剩余:0
HTTP丢包率：0/8
data[type=512,serial=006EA1B2C3D4E5202412171016470026] 入待发送队列
push data[type=512, serial=MBCP00000027, len=396] via MB FAILED, 剩余:0
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=1,serial=006EA1B2C3D4E5202412171017440027] 入待发送队列
HTTP丢包率：0/8
data[type=512,serial=006EA1B2C3D4E5202412171017480028] 入待发送队列
push data[type=1, serial=MBCP00000028, len=1013] via MB FAILED, 剩余:1
push data[type=512, serial=MBCP00000029, len=396] via MB SUCCESSED, 剩余:0
wait data[type=512, serial=006EA1B2C3D4E5202412171017480028] 响应超时(20), 丢弃
HTTP丢包率：1/9
data[type=512,serial=006EA1B2C3D4E5202412171018490029] 入待发送队列
push data[type=512, serial=MBCP00000030, len=413] via MB FAILED, 剩余:0
HTTP丢包率：1/9
data[type=512,serial=006EA1B2C3D4E5202412171019500030] 入待发送队列
push data[type=512, serial=MBCP00000031, len=413] via MB FAILED, 剩余:0
HTTP丢包率：1/9
data[type=512,serial=006EA1B2C3D4E5202412171020510031] 入待发送队列
push data[type=512, serial=MBCP00000032, len=413] via MB FAILED, 剩余:0
HTTP丢包率：1/9
data[type=512,serial=006EA1B2C3D4E5202412171021520032] 入待发送队列
push data[type=512, serial=MBCP00000033, len=413] via MB FAILED, 剩余:0
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=1,serial=006EA1B2C3D4E5202412171022440033] 入待发送队列
push data[type=1, serial=MBCP00000034, len=1036] via MB FAILED, 剩余:0
HTTP丢包率：1/9
data[type=512,serial=006EA1B2C3D4E5202412171022530034] 入待发送队列
push data[type=512, serial=MBCP00000035, len=413] via MB FAILED, 剩余:0
HTTP丢包率：1/9
data[type=512,serial=006EA1B2C3D4E5202412171023540035] 入待发送队列
push data[type=512, serial=MBCP00000036, len=413] via MB FAILED, 剩余:0
HTTP丢包率：1/9
data[type=512,serial=006EA1B2C3D4E5202412171024550036] 入待发送队列
push data[type=512, serial=MBCP00000037, len=413] via MB FAILED, 剩余:0
HTTP丢包率：1/9
data[type=512,serial=006EA1B2C3D4E5202412171025560037] 入待发送队列
push data[type=512, serial=MBCP00000038, len=413] via MB FAILED, 剩余:0
iot_status:0
RECV data from IOT, len=532
Total consumption of ink on startup：0_[K], [PRINT]S_3200, M_3200, L_3200, [FLASH]S_1640, M_1640, L_1640
Total consumption of ink on startup：1_[C], [PRINT]S_3200, M_3200, L_3200, [FLASH]S_1640, M_1640, L_1640
Total consumption of ink on startup：2_[M], [PRINT]S_3200, M_3200, L_3200, [FLASH]S_1640, M_1640, L_1640
Total consumption of ink on startup：3_[Y], [PRINT]S_3200, M_3200, L_3200, [FLASH]S_1640, M_1640, L_1640
Total consumption of ink on startup：8_[W], [PRINT]S_12800, M_12800, L_12800, [FLASH]S_6560, M_6560, L_6560
Total consumption of ink on startup：9_[V], [PRINT]S_12800, M_12800, L_12800, [FLASH]S_6560, M_6560, L_6560
RECV data from IOT, len=532
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=2,serial=006EA1B2C3D4E5202412171026440038] 入待发送队列
push data[type=2, serial=MBCP00000039, len=1017] via MB SUCCESSED, 剩余:0
iot_status:0
RECV data from IOT, len=532
作业数据(serial:0000000000, 流水:006EA1B2C3D4E5202412171026440038,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
HTTP丢包率：1/10
data[type=512,serial=006EA1B2C3D4E5202412171026570039] 入待发送队列
push data[type=512, serial=MBCP00000040, len=398] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202412171026570039,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
HTTP丢包率：1/11
data[type=512,serial=006EA1B2C3D4E5202412171027580040] 入待发送队列
push data[type=512, serial=MBCP00000041, len=413] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202412171027580040,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
HTTP丢包率：1/12
data[type=512,serial=006EA1B2C3D4E5202412171028590041] 入待发送队列
push data[type=512, serial=MBCP00000042, len=415] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202412171028590041,提交成功(0)
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
push data[type=512, serial=MBCP00000043, len=415] via MB SUCCESSED, 剩余:0
iot_status:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202412171030000042,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
Total consumption of ink on startup：0_[K], [PRINT]S_3600, M_3600, L_3600, [FLASH]S_1880, M_1880, L_1880
Total consumption of ink on startup：1_[C], [PRINT]S_3600, M_3600, L_3600, [FLASH]S_1880, M_1880, L_1880
Total consumption of ink on startup：2_[M], [PRINT]S_3600, M_3600, L_3600, [FLASH]S_1880, M_1880, L_1880
Total consumption of ink on startup：3_[Y], [PRINT]S_3600, M_3600, L_3600, [FLASH]S_1880, M_1880, L_1880
Total consumption of ink on startup：8_[W], [PRINT]S_14400, M_14400, L_14400, [FLASH]S_7520, M_7520, L_7520
Total consumption of ink on startup：9_[V], [PRINT]S_14400, M_14400, L_14400, [FLASH]S_7520, M_7520, L_7520
Total consumption of ink on startup：0_[K], [PRINT]S_4000, M_4000, L_4000, [FLASH]S_1920, M_1920, L_1920
Total consumption of ink on startup：1_[C], [PRINT]S_4000, M_4000, L_4000, [FLASH]S_1920, M_1920, L_1920
Total consumption of ink on startup：2_[M], [PRINT]S_4000, M_4000, L_4000, [FLASH]S_1920, M_1920, L_1920
Total consumption of ink on startup：3_[Y], [PRINT]S_4000, M_4000, L_4000, [FLASH]S_1920, M_1920, L_1920
Total consumption of ink on startup：8_[W], [PRINT]S_16000, M_16000, L_16000, [FLASH]S_7680, M_7680, L_7680
Total consumption of ink on startup：9_[V], [PRINT]S_16000, M_16000, L_16000, [FLASH]S_7680, M_7680, L_7680
iot_status:0
RECV data from IOT, len=532
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=2,serial=006EA1B2C3D4E5202412171030330043] 入待发送队列
push data[type=2, serial=MBCP00000044, len=1017] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
作业数据(serial:0000000000, 流水:006EA1B2C3D4E5202412171030330043,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
HTTP丢包率：1/15
data[type=512,serial=006EA1B2C3D4E5202412171031010044] 入待发送队列
push data[type=512, serial=MBCP00000045, len=415] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202412171031010044,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
Total consumption of ink on startup：0_[K], [PRINT]S_4400, M_4400, L_4400, [FLASH]S_2160, M_2160, L_2160
Total consumption of ink on startup：1_[C], [PRINT]S_4400, M_4400, L_4400, [FLASH]S_2160, M_2160, L_2160
Total consumption of ink on startup：2_[M], [PRINT]S_4400, M_4400, L_4400, [FLASH]S_2160, M_2160, L_2160
Total consumption of ink on startup：3_[Y], [PRINT]S_4400, M_4400, L_4400, [FLASH]S_2160, M_2160, L_2160
Total consumption of ink on startup：8_[W], [PRINT]S_17600, M_17600, L_17600, [FLASH]S_8640, M_8640, L_8640
Total consumption of ink on startup：9_[V], [PRINT]S_17600, M_17600, L_17600, [FLASH]S_8640, M_8640, L_8640
iot_status:0
RECV data from IOT, len=532
HTTP丢包率：1/16
data[type=512,serial=006EA1B2C3D4E5202412171032020045] 入待发送队列
push data[type=512, serial=MBCP00000046, len=401] via MB FAILED, 剩余:0
HTTP丢包率：1/16
data[type=512,serial=006EA1B2C3D4E5202412171033040046] 入待发送队列
push data[type=512, serial=MBCP00000047, len=401] via MB FAILED, 剩余:0
HTTP丢包率：1/16
data[type=512,serial=006EA1B2C3D4E5202412171034050047] 入待发送队列
push data[type=512, serial=MBCP00000048, len=401] via MB FAILED, 剩余:0
HTTP丢包率：1/16
data[type=512,serial=006EA1B2C3D4E5202412171035060048] 入待发送队列
push data[type=512, serial=MBCP00000049, len=401] via MB FAILED, 剩余:0
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=1,serial=006EA1B2C3D4E5202412171035580049] 入待发送队列
push data[type=1, serial=MBCP00000050, len=978] via MB FAILED, 剩余:0
HTTP丢包率：1/16
data[type=512,serial=006EA1B2C3D4E5202412171036070050] 入待发送队列
push data[type=512, serial=MBCP00000051, len=401] via MB FAILED, 剩余:0
HTTP丢包率：1/16
data[type=512,serial=006EA1B2C3D4E5202412171037080051] 入待发送队列
push data[type=512, serial=MBCP00000052, len=401] via MB FAILED, 剩余:0
HTTP丢包率：1/16
data[type=512,serial=006EA1B2C3D4E5202412171038090052] 入待发送队列
push data[type=512, serial=MBCP00000053, len=401] via MB FAILED, 剩余:0
HTTP丢包率：1/16
data[type=512,serial=006EA1B2C3D4E5202412171039100053] 入待发送队列
push data[type=512, serial=MBCP00000054, len=401] via MB FAILED, 剩余:0
HTTP丢包率：1/16
data[type=512,serial=006EA1B2C3D4E5202412171040110054] 入待发送队列
push data[type=512, serial=MBCP00000055, len=401] via MB FAILED, 剩余:0
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=1,serial=006EA1B2C3D4E5202412171040580055] 入待发送队列
push data[type=1, serial=MBCP00000056, len=978] via MB FAILED, 剩余:0
HTTP丢包率：1/16
data[type=512,serial=006EA1B2C3D4E5202412171041120056] 入待发送队列
push data[type=512, serial=MBCP00000057, len=401] via MB FAILED, 剩余:0
HTTP丢包率：1/16
data[type=512,serial=006EA1B2C3D4E5202412171042130057] 入待发送队列
push data[type=512, serial=MBCP00000058, len=401] via MB FAILED, 剩余:0
HTTP丢包率：1/16
data[type=512,serial=006EA1B2C3D4E5202412171043140058] 入待发送队列
push data[type=512, serial=MBCP00000059, len=401] via MB FAILED, 剩余:0
HTTP丢包率：1/16
data[type=512,serial=006EA1B2C3D4E5202412171044150059] 入待发送队列
push data[type=512, serial=MBCP00000060, len=401] via MB FAILED, 剩余:0
HTTP丢包率：1/16
data[type=512,serial=006EA1B2C3D4E5202412171045160060] 入待发送队列
push data[type=512, serial=MBCP00000061, len=401] via MB FAILED, 剩余:0
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=1,serial=006EA1B2C3D4E5202412171045580061] 入待发送队列
push data[type=1, serial=MBCP00000062, len=978] via MB FAILED, 剩余:0
HTTP丢包率：1/16
data[type=512,serial=006EA1B2C3D4E5202412171046170062] 入待发送队列
push data[type=512, serial=MBCP00000063, len=401] via MB FAILED, 剩余:0
HTTP丢包率：1/16
data[type=512,serial=006EA1B2C3D4E5202412171047180063] 入待发送队列
push data[type=512, serial=MBCP00000064, len=401] via MB FAILED, 剩余:0
HTTP丢包率：1/16
data[type=512,serial=006EA1B2C3D4E5202412171048190064] 入待发送队列
push data[type=512, serial=MBCP00000065, len=401] via MB FAILED, 剩余:0
HTTP丢包率：1/16
data[type=512,serial=006EA1B2C3D4E5202412171049200065] 入待发送队列
push data[type=512, serial=MBCP00000066, len=401] via MB FAILED, 剩余:0
HTTP丢包率：1/16
data[type=512,serial=006EA1B2C3D4E5202412171050210066] 入待发送队列
push data[type=512, serial=MBCP00000067, len=401] via MB FAILED, 剩余:0
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=1,serial=006EA1B2C3D4E5202412171050580067] 入待发送队列
push data[type=1, serial=MBCP00000068, len=978] via MB FAILED, 剩余:0
HTTP丢包率：1/16
data[type=512,serial=006EA1B2C3D4E5202412171051220068] 入待发送队列
push data[type=512, serial=MBCP00000069, len=401] via MB FAILED, 剩余:0
HTTP丢包率：1/16
data[type=512,serial=006EA1B2C3D4E5202412171052230069] 入待发送队列
push data[type=512, serial=MBCP00000070, len=401] via MB FAILED, 剩余:0
HTTP丢包率：1/16
data[type=512,serial=006EA1B2C3D4E5202412171053240070] 入待发送队列
push data[type=512, serial=MBCP00000071, len=401] via MB FAILED, 剩余:0
HTTP丢包率：1/16
data[type=512,serial=006EA1B2C3D4E5202412171054250071] 入待发送队列
push data[type=512, serial=MBCP00000072, len=401] via MB FAILED, 剩余:0
HTTP丢包率：1/16
data[type=512,serial=006EA1B2C3D4E5202412171055260072] 入待发送队列
push data[type=512, serial=MBCP00000073, len=401] via MB FAILED, 剩余:0
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=1,serial=006EA1B2C3D4E5202412171055580073] 入待发送队列
push data[type=1, serial=MBCP00000074, len=978] via MB FAILED, 剩余:0
HTTP丢包率：1/16
data[type=512,serial=006EA1B2C3D4E5202412171056270074] 入待发送队列
push data[type=512, serial=MBCP00000075, len=401] via MB FAILED, 剩余:0
HTTP丢包率：1/16
data[type=512,serial=006EA1B2C3D4E5202412171057280075] 入待发送队列
push data[type=512, serial=MBCP00000076, len=401] via MB FAILED, 剩余:0
HTTP丢包率：1/16
data[type=512,serial=006EA1B2C3D4E5202412171058290076] 入待发送队列
push data[type=512, serial=MBCP00000077, len=401] via MB FAILED, 剩余:0
HTTP丢包率：1/16
data[type=512,serial=006EA1B2C3D4E5202412171059300077] 入待发送队列
push data[type=512, serial=MBCP00000078, len=401] via MB FAILED, 剩余:0
HTTP丢包率：1/16
data[type=512,serial=006EA1B2C3D4E5202412171100310078] 入待发送队列
push data[type=512, serial=MBCP00000079, len=401] via MB FAILED, 剩余:0
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=1,serial=006EA1B2C3D4E5202412171100580079] 入待发送队列
push data[type=1, serial=MBCP00000080, len=978] via MB FAILED, 剩余:0
HTTP丢包率：1/16
data[type=512,serial=006EA1B2C3D4E5202412171101320080] 入待发送队列
push data[type=512, serial=MBCP00000081, len=401] via MB FAILED, 剩余:0
HTTP丢包率：1/16
data[type=512,serial=006EA1B2C3D4E5202412171102330081] 入待发送队列
push data[type=512, serial=MBCP00000082, len=401] via MB FAILED, 剩余:0
HTTP丢包率：1/16
data[type=512,serial=006EA1B2C3D4E5202412171103340082] 入待发送队列
push data[type=512, serial=MBCP00000083, len=401] via MB FAILED, 剩余:0
HTTP丢包率：1/16
data[type=512,serial=006EA1B2C3D4E5202412171104350083] 入待发送队列
push data[type=512, serial=MBCP00000084, len=401] via MB FAILED, 剩余:0
HTTP丢包率：1/16
data[type=512,serial=006EA1B2C3D4E5202412171105360084] 入待发送队列
push data[type=512, serial=MBCP00000085, len=401] via MB FAILED, 剩余:0
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=1,serial=006EA1B2C3D4E5202412171105580085] 入待发送队列
push data[type=1, serial=MBCP00000086, len=978] via MB FAILED, 剩余:0
HTTP丢包率：1/16
data[type=512,serial=006EA1B2C3D4E5202412171106370086] 入待发送队列
push data[type=512, serial=MBCP00000087, len=401] via MB FAILED, 剩余:0
HTTP丢包率：1/16
data[type=512,serial=006EA1B2C3D4E5202412171107380087] 入待发送队列
push data[type=512, serial=MBCP00000088, len=401] via MB FAILED, 剩余:0
HTTP丢包率：1/16
data[type=512,serial=006EA1B2C3D4E5202412171108390088] 入待发送队列
push data[type=512, serial=MBCP00000089, len=401] via MB FAILED, 剩余:0
HTTP丢包率：1/16
data[type=512,serial=006EA1B2C3D4E5202412171109400089] 入待发送队列
push data[type=512, serial=MBCP00000090, len=401] via MB FAILED, 剩余:0
HTTP丢包率：1/16
data[type=512,serial=006EA1B2C3D4E5202412171110410090] 入待发送队列
push data[type=512, serial=MBCP00000091, len=401] via MB FAILED, 剩余:0
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=1,serial=006EA1B2C3D4E5202412171110580091] 入待发送队列
push data[type=1, serial=MBCP00000092, len=978] via MB FAILED, 剩余:0
HTTP丢包率：1/16
data[type=512,serial=006EA1B2C3D4E5202412171111420092] 入待发送队列
push data[type=512, serial=MBCP00000093, len=401] via MB FAILED, 剩余:0
HTTP丢包率：1/16
data[type=512,serial=006EA1B2C3D4E5202412171112430093] 入待发送队列
push data[type=512, serial=MBCP00000094, len=401] via MB FAILED, 剩余:0
HTTP丢包率：1/16
data[type=512,serial=006EA1B2C3D4E5202412171113440094] 入待发送队列
push data[type=512, serial=MBCP00000095, len=401] via MB FAILED, 剩余:0
HTTP丢包率：1/16
data[type=512,serial=006EA1B2C3D4E5202412171114450095] 入待发送队列
push data[type=512, serial=MBCP00000096, len=401] via MB FAILED, 剩余:0
HTTP丢包率：1/16
data[type=512,serial=006EA1B2C3D4E5202412171115460096] 入待发送队列
push data[type=512, serial=MBCP00000097, len=401] via MB FAILED, 剩余:0
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=1,serial=006EA1B2C3D4E5202412171115580097] 入待发送队列
push data[type=1, serial=MBCP00000098, len=978] via MB FAILED, 剩余:0
HTTP丢包率：1/16
data[type=512,serial=006EA1B2C3D4E5202412171116470098] 入待发送队列
push data[type=512, serial=MBCP00000099, len=401] via MB FAILED, 剩余:0
HTTP丢包率：1/16
data[type=512,serial=006EA1B2C3D4E5202412171117480099] 入待发送队列
push data[type=512, serial=MBCP00000100, len=401] via MB FAILED, 剩余:0
HTTP丢包率：1/16
data[type=512,serial=006EA1B2C3D4E5202412171118490100] 入待发送队列
push data[type=512, serial=MBCP00000101, len=401] via MB FAILED, 剩余:0
HTTP丢包率：1/16
data[type=512,serial=006EA1B2C3D4E5202412171119500101] 入待发送队列
push data[type=512, serial=MBCP00000102, len=401] via MB FAILED, 剩余:0
HTTP丢包率：1/16
data[type=512,serial=006EA1B2C3D4E5202412171120510102] 入待发送队列
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=1,serial=006EA1B2C3D4E5202412171120580103] 入待发送队列
push data[type=512, serial=MBCP00000103, len=401] via MB FAILED, 剩余:1
push data[type=1, serial=MBCP00000104, len=978] via MB FAILED, 剩余:0
云模块版本:2.1.0.0
DATA SUBCRIBER:[CLOUD_PLATFORM,]
iot_status:3
iot_status:3
iot_status:3
The mainboard is not initialized. 
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
The mainboard is not initialized. 
The mainboard is not initialized. 
The mainboard is not initialized. 
Total consumption of ink on startup：0_[K], [PRINT]S_204040, M_1064, L_237552, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_204040, M_1064, L_237552, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_204948, M_1064, L_237552, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_204040, M_1064, L_237552, [FLASH]S_0, M_0, L_0
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=2,serial=FFFFFFFF202412171135000000] 入待发送队列
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
CLOUD_PLATFORM线程退出
The mainboard is not initialized. 
CloudServiceCore线程退出
