云模块版本:2.1.0.0
DATA SUBCRIBER:[CLOUD_PLATFORM,]
CLOUD_PLATFORM线程退出
CloudServiceCore线程退出
云模块版本:2.1.0.0
DATA SUBCRIBER:[CLOUD_PLATFORM,]
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
server-addr:http://pt.hosonsoft.com:5000/footstone-server/api/kdata
HTTP丢包率：0/0
data[type=512,serial=006EA1B2C3D4E5202412161435560000] 入待发送队列
iot_ccid:CCID-123, imei:IMEI-123
push data[type=512, serial=MBCP00000001, len=386] via MB SUCCESSED, 剩余:0
data[type=256,serial=006EA1B2C3D4E5202412161435560001] 入待发送队列
data[type=128,serial=006EA1B2C3D4E5202412161435560002] 入待发送队列
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202412161435560000,提交成功(0)
push data[type=128, serial=MBCP00000002, len=404] via MB SUCCESSED, 剩余:1
iot_status:0
RECV data from IOT, len=532
iot基站数据(serial:0000000000, 流水:006EA1B2C3D4E5202412161435560002,提交成功(0)
push data[type=256, serial=MBCP00000003, len=468] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
iot-sim数据(serial:0000000000, 流水:006EA1B2C3D4E5202412161435560001,提交成功(0)
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
CLOUD_PLATFORM线程退出
CloudServiceCore线程退出
云模块版本:2.1.0.0
DATA SUBCRIBER:[CLOUD_PLATFORM,]
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
server-addr:http://pt.hosonsoft.com:5000/footstone-server/api/kdata
HTTP丢包率：0/0
data[type=512,serial=006EA1B2C3D4E5202412161436420000] 入待发送队列
data[type=256,serial=006EA1B2C3D4E5202412161436420001] 入待发送队列
iot_ccid:CCID-123, imei:IMEI-123
push data[type=256, serial=MBCP00000001, len=468] via MB SUCCESSED, 剩余:1
data[type=128,serial=006EA1B2C3D4E5202412161436420002] 入待发送队列
RECV data from IOT, len=532
iot-sim数据(serial:0000000000, 流水:006EA1B2C3D4E5202412161436420001,提交成功(0)
push data[type=128, serial=MBCP00000002, len=404] via MB SUCCESSED, 剩余:1
RECV data from IOT, len=532
iot基站数据(serial:0000000000, 流水:006EA1B2C3D4E5202412161436420002,提交成功(0)
push data[type=512, serial=MBCP00000003, len=386] via MB SUCCESSED, 剩余:0
iot_status:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202412161436420000,提交成功(0)
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
HTTP丢包率：0/3
data[type=512,serial=006EA1B2C3D4E5202412161437430003] 入待发送队列
push data[type=512, serial=MBCP00000004, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202412161437430003,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
HTTP丢包率：0/4
data[type=512,serial=006EA1B2C3D4E5202412161438440004] 入待发送队列
push data[type=512, serial=MBCP00000005, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202412161438440004,提交成功(0)
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
HTTP丢包率：0/5
data[type=512,serial=006EA1B2C3D4E5202412161439450005] 入待发送队列
push data[type=512, serial=MBCP00000006, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202412161439450005,提交成功(0)
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
HTTP丢包率：0/6
data[type=512,serial=006EA1B2C3D4E5202412161440460006] 入待发送队列
push data[type=512, serial=MBCP00000007, len=396] via MB SUCCESSED, 剩余:0
iot_status:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202412161440460006,提交成功(0)
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
HTTP丢包率：0/7
data[type=512,serial=006EA1B2C3D4E5202412161441470007] 入待发送队列
push data[type=512, serial=MBCP00000008, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202412161441470007,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
HTTP丢包率：0/8
data[type=512,serial=006EA1B2C3D4E5202412161442480008] 入待发送队列
push data[type=512, serial=MBCP00000009, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202412161442480008,提交成功(0)
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
HTTP丢包率：0/9
data[type=512,serial=006EA1B2C3D4E5202412161443490009] 入待发送队列
push data[type=512, serial=MBCP00000010, len=396] via MB SUCCESSED, 剩余:0
iot_status:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202412161443490009,提交成功(0)
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
CLOUD_PLATFORM线程退出
CloudServiceCore线程退出
云模块版本:2.1.0.0
DATA SUBCRIBER:[CLOUD_PLATFORM,]
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
server-addr:http://pt.hosonsoft.com:5000/footstone-server/api/kdata
HTTP丢包率：0/0
data[type=512,serial=006EA1B2C3D4E5202412161618590000] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_200, M_200, L_200
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_200, M_200, L_200
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_200, M_200, L_200
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_200, M_200, L_200
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_800, M_800, L_800
Total consumption of ink on startup：9_[V], [PRINT]S_0, M_0, L_0, [FLASH]S_800, M_800, L_800
iot_ccid:CCID-123, imei:IMEI-123
push data[type=512, serial=MBCP00000001, len=386] via MB SUCCESSED, 剩余:0
data[type=256,serial=006EA1B2C3D4E5202412161618590001] 入待发送队列
data[type=128,serial=006EA1B2C3D4E5202412161618590002] 入待发送队列
iot_status:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202412161618590000,提交成功(0)
push data[type=128, serial=MBCP00000002, len=404] via MB SUCCESSED, 剩余:1
RECV data from IOT, len=532
iot基站数据(serial:0000000000, 流水:006EA1B2C3D4E5202412161618590002,提交成功(0)
push data[type=256, serial=MBCP00000003, len=468] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
iot-sim数据(serial:0000000000, 流水:006EA1B2C3D4E5202412161618590001,提交成功(0)
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
push data[type=512, serial=MBCP00000004, len=396] via MB SUCCESSED, 剩余:0
iot_status:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202412161620000003,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
CLOUD_PLATFORM线程退出
CloudServiceCore线程退出
云模块版本:2.1.0.0
DATA SUBCRIBER:[CLOUD_PLATFORM,]
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
server-addr:http://pt.hosonsoft.com:5000/footstone-server/api/kdata
HTTP丢包率：0/0
data[type=512,serial=006EA1B2C3D4E5202412161622490000] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_440, M_440, L_440
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_440, M_440, L_440
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_440, M_440, L_440
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_440, M_440, L_440
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_1760, M_1760, L_1760
Total consumption of ink on startup：9_[V], [PRINT]S_0, M_0, L_0, [FLASH]S_1760, M_1760, L_1760
iot_ccid:CCID-123, imei:IMEI-123
data[type=256,serial=006EA1B2C3D4E5202412161622490001] 入待发送队列
data[type=128,serial=006EA1B2C3D4E5202412161622490002] 入待发送队列
iot_status:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202412161622490000,提交成功(0)
push data[type=128, serial=MBCP00000002, len=404] via MB SUCCESSED, 剩余:1
RECV data from IOT, len=532
iot基站数据(serial:0000000000, 流水:006EA1B2C3D4E5202412161622490002,提交成功(0)
push data[type=256, serial=MBCP00000003, len=468] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
iot-sim数据(serial:0000000000, 流水:006EA1B2C3D4E5202412161622490001,提交成功(0)
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
HTTP丢包率：0/3
data[type=512,serial=006EA1B2C3D4E5202412161623500003] 入待发送队列
iot_status:0
push data[type=512, serial=MBCP00000004, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202412161623500003,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
Total consumption of ink on startup：0_[K], [PRINT]S_400, M_400, L_400, [FLASH]S_680, M_680, L_680
Total consumption of ink on startup：1_[C], [PRINT]S_400, M_400, L_400, [FLASH]S_680, M_680, L_680
Total consumption of ink on startup：2_[M], [PRINT]S_400, M_400, L_400, [FLASH]S_680, M_680, L_680
Total consumption of ink on startup：3_[Y], [PRINT]S_400, M_400, L_400, [FLASH]S_680, M_680, L_680
Total consumption of ink on startup：8_[W], [PRINT]S_1600, M_1600, L_1600, [FLASH]S_2720, M_2720, L_2720
Total consumption of ink on startup：9_[V], [PRINT]S_1600, M_1600, L_1600, [FLASH]S_2720, M_2720, L_2720
Total consumption of ink on startup：0_[K], [PRINT]S_800, M_800, L_800, [FLASH]S_720, M_720, L_720
Total consumption of ink on startup：1_[C], [PRINT]S_800, M_800, L_800, [FLASH]S_720, M_720, L_720
Total consumption of ink on startup：2_[M], [PRINT]S_800, M_800, L_800, [FLASH]S_720, M_720, L_720
Total consumption of ink on startup：3_[Y], [PRINT]S_800, M_800, L_800, [FLASH]S_720, M_720, L_720
Total consumption of ink on startup：8_[W], [PRINT]S_3200, M_3200, L_3200, [FLASH]S_2880, M_2880, L_2880
Total consumption of ink on startup：9_[V], [PRINT]S_3200, M_3200, L_3200, [FLASH]S_2880, M_2880, L_2880
iot_status:0
RECV data from IOT, len=532
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=2,serial=006EA1B2C3D4E5202412161624200004] 入待发送队列
push data[type=2, serial=MBCP00000005, len=1017] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
作业数据(serial:0000000000, 流水:006EA1B2C3D4E5202412161624200004,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
HTTP丢包率：0/5
data[type=512,serial=006EA1B2C3D4E5202412161624510005] 入待发送队列
push data[type=512, serial=MBCP00000006, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202412161624510005,提交成功(0)
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
CLOUD_PLATFORM线程退出
CloudServiceCore线程退出
云模块版本:2.1.0.0
DATA SUBCRIBER:[CLOUD_PLATFORM,]
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
server-addr:http://pt.hosonsoft.com:5000/footstone-server/api/kdata
HTTP丢包率：0/0
data[type=512,serial=006EA1B2C3D4E5202412161628380000] 入待发送队列
data[type=256,serial=006EA1B2C3D4E5202412161628380001] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_800, M_800, L_800, [FLASH]S_840, M_840, L_840
Total consumption of ink on startup：1_[C], [PRINT]S_800, M_800, L_800, [FLASH]S_840, M_840, L_840
Total consumption of ink on startup：2_[M], [PRINT]S_800, M_800, L_800, [FLASH]S_840, M_840, L_840
Total consumption of ink on startup：3_[Y], [PRINT]S_800, M_800, L_800, [FLASH]S_840, M_840, L_840
Total consumption of ink on startup：8_[W], [PRINT]S_3200, M_3200, L_3200, [FLASH]S_3360, M_3360, L_3360
Total consumption of ink on startup：9_[V], [PRINT]S_3200, M_3200, L_3200, [FLASH]S_3360, M_3360, L_3360
iot_ccid:CCID-123, imei:IMEI-123
push data[type=256, serial=MBCP00000001, len=468] via MB SUCCESSED, 剩余:1
data[type=128,serial=006EA1B2C3D4E5202412161628390002] 入待发送队列
RECV data from IOT, len=532
iot-sim数据(serial:0000000000, 流水:006EA1B2C3D4E5202412161628380001,提交成功(0)
push data[type=128, serial=MBCP00000002, len=404] via MB SUCCESSED, 剩余:1
RECV data from IOT, len=532
iot基站数据(serial:0000000000, 流水:006EA1B2C3D4E5202412161628390002,提交成功(0)
push data[type=512, serial=MBCP00000003, len=386] via MB SUCCESSED, 剩余:0
iot_status:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202412161628380000,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
Total consumption of ink on startup：0_[K], [PRINT]S_1200, M_1200, L_1200, [FLASH]S_1080, M_1080, L_1080
Total consumption of ink on startup：1_[C], [PRINT]S_1200, M_1200, L_1200, [FLASH]S_1080, M_1080, L_1080
Total consumption of ink on startup：2_[M], [PRINT]S_1200, M_1200, L_1200, [FLASH]S_1080, M_1080, L_1080
Total consumption of ink on startup：3_[Y], [PRINT]S_1200, M_1200, L_1200, [FLASH]S_1080, M_1080, L_1080
Total consumption of ink on startup：8_[W], [PRINT]S_4800, M_4800, L_4800, [FLASH]S_4320, M_4320, L_4320
Total consumption of ink on startup：9_[V], [PRINT]S_4800, M_4800, L_4800, [FLASH]S_4320, M_4320, L_4320
RECV data from IOT, len=532
Total consumption of ink on startup：0_[K], [PRINT]S_1600, M_1600, L_1600, [FLASH]S_1120, M_1120, L_1120
Total consumption of ink on startup：1_[C], [PRINT]S_1600, M_1600, L_1600, [FLASH]S_1120, M_1120, L_1120
Total consumption of ink on startup：2_[M], [PRINT]S_1600, M_1600, L_1600, [FLASH]S_1120, M_1120, L_1120
Total consumption of ink on startup：3_[Y], [PRINT]S_1600, M_1600, L_1600, [FLASH]S_1120, M_1120, L_1120
Total consumption of ink on startup：8_[W], [PRINT]S_6400, M_6400, L_6400, [FLASH]S_4480, M_4480, L_4480
Total consumption of ink on startup：9_[V], [PRINT]S_6400, M_6400, L_6400, [FLASH]S_4480, M_4480, L_4480
iot_status:0
RECV data from IOT, len=532
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=2,serial=006EA1B2C3D4E5202412161629070003] 入待发送队列
push data[type=2, serial=MBCP00000004, len=1017] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
作业数据(serial:0000000000, 流水:006EA1B2C3D4E5202412161629070003,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
HTTP丢包率：0/4
data[type=512,serial=006EA1B2C3D4E5202412161629390004] 入待发送队列
push data[type=512, serial=MBCP00000005, len=396] via MB SUCCESSED, 剩余:0
iot_status:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202412161629390004,提交成功(0)
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
HTTP丢包率：0/5
data[type=512,serial=006EA1B2C3D4E5202412161630400005] 入待发送队列
push data[type=512, serial=MBCP00000006, len=396] via MB FAILED, 剩余:0
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
Total consumption of ink on startup：0_[K], [PRINT]S_2000, M_2000, L_2000, [FLASH]S_1360, M_1360, L_1360
Total consumption of ink on startup：1_[C], [PRINT]S_2000, M_2000, L_2000, [FLASH]S_1360, M_1360, L_1360
Total consumption of ink on startup：2_[M], [PRINT]S_2000, M_2000, L_2000, [FLASH]S_1360, M_1360, L_1360
Total consumption of ink on startup：3_[Y], [PRINT]S_2000, M_2000, L_2000, [FLASH]S_1360, M_1360, L_1360
Total consumption of ink on startup：8_[W], [PRINT]S_8000, M_8000, L_8000, [FLASH]S_5440, M_5440, L_5440
Total consumption of ink on startup：9_[V], [PRINT]S_8000, M_8000, L_8000, [FLASH]S_5440, M_5440, L_5440
Total consumption of ink on startup：0_[K], [PRINT]S_2400, M_2400, L_2400, [FLASH]S_1400, M_1400, L_1400
Total consumption of ink on startup：1_[C], [PRINT]S_2400, M_2400, L_2400, [FLASH]S_1400, M_1400, L_1400
Total consumption of ink on startup：2_[M], [PRINT]S_2400, M_2400, L_2400, [FLASH]S_1400, M_1400, L_1400
Total consumption of ink on startup：3_[Y], [PRINT]S_2400, M_2400, L_2400, [FLASH]S_1400, M_1400, L_1400
Total consumption of ink on startup：8_[W], [PRINT]S_9600, M_9600, L_9600, [FLASH]S_5600, M_5600, L_5600
Total consumption of ink on startup：9_[V], [PRINT]S_9600, M_9600, L_9600, [FLASH]S_5600, M_5600, L_5600
iot_status:0
RECV data from IOT, len=532
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=2,serial=006EA1B2C3D4E5202412161631160006] 入待发送队列
push data[type=2, serial=MBCP00000007, len=998] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
作业数据(serial:0000000000, 流水:006EA1B2C3D4E5202412161631160006,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
HTTP丢包率：0/6
data[type=512,serial=006EA1B2C3D4E5202412161631410007] 入待发送队列
push data[type=512, serial=MBCP00000008, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202412161631410007,提交成功(0)
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
HTTP丢包率：0/7
data[type=512,serial=006EA1B2C3D4E5202412161632420008] 入待发送队列
push data[type=512, serial=MBCP00000009, len=396] via MB SUCCESSED, 剩余:0
iot_status:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202412161632420008,提交成功(0)
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
HTTP丢包率：0/8
data[type=512,serial=006EA1B2C3D4E5202412161633430009] 入待发送队列
push data[type=512, serial=MBCP00000010, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202412161633430009,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
CLOUD_PLATFORM线程退出
CloudServiceCore线程退出
云模块版本:2.1.0.0
DATA SUBCRIBER:[CLOUD_PLATFORM,]
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
server-addr:http://pt.hosonsoft.com:5000/footstone-server/api/kdata
HTTP丢包率：0/0
data[type=512,serial=006EA1B2C3D4E5202412161638140000] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_2400, M_2400, L_2400, [FLASH]S_1520, M_1520, L_1520
Total consumption of ink on startup：1_[C], [PRINT]S_2400, M_2400, L_2400, [FLASH]S_1520, M_1520, L_1520
Total consumption of ink on startup：2_[M], [PRINT]S_2400, M_2400, L_2400, [FLASH]S_1520, M_1520, L_1520
Total consumption of ink on startup：3_[Y], [PRINT]S_2400, M_2400, L_2400, [FLASH]S_1520, M_1520, L_1520
Total consumption of ink on startup：8_[W], [PRINT]S_9600, M_9600, L_9600, [FLASH]S_6080, M_6080, L_6080
Total consumption of ink on startup：9_[V], [PRINT]S_9600, M_9600, L_9600, [FLASH]S_6080, M_6080, L_6080
iot_ccid:CCID-123, imei:IMEI-123
push data[type=512, serial=MBCP00000001, len=386] via MB SUCCESSED, 剩余:0
data[type=256,serial=006EA1B2C3D4E5202412161638140001] 入待发送队列
data[type=128,serial=006EA1B2C3D4E5202412161638140002] 入待发送队列
iot_status:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202412161638140000,提交成功(0)
push data[type=128, serial=MBCP00000002, len=404] via MB SUCCESSED, 剩余:1
RECV data from IOT, len=532
iot基站数据(serial:0000000000, 流水:006EA1B2C3D4E5202412161638140002,提交成功(0)
push data[type=256, serial=MBCP00000003, len=468] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
iot-sim数据(serial:0000000000, 流水:006EA1B2C3D4E5202412161638140001,提交成功(0)
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
Total consumption of ink on startup：0_[K], [PRINT]S_2800, M_2800, L_2800, [FLASH]S_1760, M_1760, L_1760
Total consumption of ink on startup：1_[C], [PRINT]S_2800, M_2800, L_2800, [FLASH]S_1760, M_1760, L_1760
Total consumption of ink on startup：2_[M], [PRINT]S_2800, M_2800, L_2800, [FLASH]S_1760, M_1760, L_1760
Total consumption of ink on startup：3_[Y], [PRINT]S_2800, M_2800, L_2800, [FLASH]S_1760, M_1760, L_1760
Total consumption of ink on startup：8_[W], [PRINT]S_11200, M_11200, L_11200, [FLASH]S_7040, M_7040, L_7040
Total consumption of ink on startup：9_[V], [PRINT]S_11200, M_11200, L_11200, [FLASH]S_7040, M_7040, L_7040
Total consumption of ink on startup：0_[K], [PRINT]S_3200, M_3200, L_3200, [FLASH]S_1800, M_1800, L_1800
Total consumption of ink on startup：1_[C], [PRINT]S_3200, M_3200, L_3200, [FLASH]S_1800, M_1800, L_1800
Total consumption of ink on startup：2_[M], [PRINT]S_3200, M_3200, L_3200, [FLASH]S_1800, M_1800, L_1800
Total consumption of ink on startup：3_[Y], [PRINT]S_3200, M_3200, L_3200, [FLASH]S_1800, M_1800, L_1800
Total consumption of ink on startup：8_[W], [PRINT]S_12800, M_12800, L_12800, [FLASH]S_7200, M_7200, L_7200
Total consumption of ink on startup：9_[V], [PRINT]S_12800, M_12800, L_12800, [FLASH]S_7200, M_7200, L_7200
iot_status:0
RECV data from IOT, len=532
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=2,serial=006EA1B2C3D4E5202412161638390003] 入待发送队列
push data[type=2, serial=MBCP00000004, len=1017] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
作业数据(serial:0000000000, 流水:006EA1B2C3D4E5202412161638390003,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
HTTP丢包率：0/4
data[type=512,serial=006EA1B2C3D4E5202412161639150004] 入待发送队列
push data[type=512, serial=MBCP00000005, len=396] via MB FAILED, 剩余:0
HTTP丢包率：0/4
data[type=512,serial=006EA1B2C3D4E5202412161640160005] 入待发送队列
push data[type=512, serial=MBCP00000006, len=396] via MB FAILED, 剩余:0
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
Total consumption of ink on startup：0_[K], [PRINT]S_3600, M_3600, L_3600, [FLASH]S_2040, M_2040, L_2040
Total consumption of ink on startup：1_[C], [PRINT]S_3600, M_3600, L_3600, [FLASH]S_2040, M_2040, L_2040
Total consumption of ink on startup：2_[M], [PRINT]S_3600, M_3600, L_3600, [FLASH]S_2040, M_2040, L_2040
Total consumption of ink on startup：3_[Y], [PRINT]S_3600, M_3600, L_3600, [FLASH]S_2040, M_2040, L_2040
Total consumption of ink on startup：8_[W], [PRINT]S_14400, M_14400, L_14400, [FLASH]S_8160, M_8160, L_8160
Total consumption of ink on startup：9_[V], [PRINT]S_14400, M_14400, L_14400, [FLASH]S_8160, M_8160, L_8160
iot_status:0
RECV data from IOT, len=532
Total consumption of ink on startup：0_[K], [PRINT]S_4000, M_4000, L_4000, [FLASH]S_2080, M_2080, L_2080
Total consumption of ink on startup：1_[C], [PRINT]S_4000, M_4000, L_4000, [FLASH]S_2080, M_2080, L_2080
Total consumption of ink on startup：2_[M], [PRINT]S_4000, M_4000, L_4000, [FLASH]S_2080, M_2080, L_2080
Total consumption of ink on startup：3_[Y], [PRINT]S_4000, M_4000, L_4000, [FLASH]S_2080, M_2080, L_2080
Total consumption of ink on startup：8_[W], [PRINT]S_16000, M_16000, L_16000, [FLASH]S_8320, M_8320, L_8320
Total consumption of ink on startup：9_[V], [PRINT]S_16000, M_16000, L_16000, [FLASH]S_8320, M_8320, L_8320
RECV data from IOT, len=532
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=2,serial=006EA1B2C3D4E5202412161641120006] 入待发送队列
push data[type=2, serial=MBCP00000007, len=998] via MB SUCCESSED, 剩余:0
iot_status:0
RECV data from IOT, len=532
作业数据(serial:0000000000, 流水:006EA1B2C3D4E5202412161641120006,提交成功(0)
RECV data from IOT, len=532
HTTP丢包率：0/5
data[type=512,serial=006EA1B2C3D4E5202412161641170007] 入待发送队列
push data[type=512, serial=MBCP00000008, len=396] via MB SUCCESSED, 剩余:0
iot_status:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202412161641170007,提交成功(0)
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
Total consumption of ink on startup：0_[K], [PRINT]S_4400, M_4400, L_4400, [FLASH]S_2320, M_2320, L_2320
Total consumption of ink on startup：1_[C], [PRINT]S_4400, M_4400, L_4400, [FLASH]S_2320, M_2320, L_2320
Total consumption of ink on startup：2_[M], [PRINT]S_4400, M_4400, L_4400, [FLASH]S_2320, M_2320, L_2320
Total consumption of ink on startup：3_[Y], [PRINT]S_4400, M_4400, L_4400, [FLASH]S_2320, M_2320, L_2320
Total consumption of ink on startup：8_[W], [PRINT]S_17600, M_17600, L_17600, [FLASH]S_9280, M_9280, L_9280
Total consumption of ink on startup：9_[V], [PRINT]S_17600, M_17600, L_17600, [FLASH]S_9280, M_9280, L_9280
iot_status:0
RECV data from IOT, len=532
HTTP丢包率：0/6
data[type=512,serial=006EA1B2C3D4E5202412161642180008] 入待发送队列
push data[type=512, serial=MBCP00000009, len=396] via MB SUCCESSED, 剩余:0
wait data[type=512, serial=006EA1B2C3D4E5202412161642180008] 响应超时(20), 丢弃
HTTP丢包率：1/7
data[type=512,serial=006EA1B2C3D4E5202412161643190009] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_4800, M_4800, L_4800, [FLASH]S_2360, M_2360, L_2360
Total consumption of ink on startup：1_[C], [PRINT]S_4800, M_4800, L_4800, [FLASH]S_2360, M_2360, L_2360
Total consumption of ink on startup：2_[M], [PRINT]S_4800, M_4800, L_4800, [FLASH]S_2360, M_2360, L_2360
Total consumption of ink on startup：3_[Y], [PRINT]S_4800, M_4800, L_4800, [FLASH]S_2360, M_2360, L_2360
Total consumption of ink on startup：8_[W], [PRINT]S_19200, M_19200, L_19200, [FLASH]S_9440, M_9440, L_9440
Total consumption of ink on startup：9_[V], [PRINT]S_19200, M_19200, L_19200, [FLASH]S_9440, M_9440, L_9440
push data[type=512, serial=MBCP00000010, len=414] via MB SUCCESSED, 剩余:0
iot_status:0
RECV data from IOT, len=532
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=2,serial=006EA1B2C3D4E5202412161643210010] 入待发送队列
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=1,serial=006EA1B2C3D4E5202412161643210011] 入待发送队列
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202412161643190009,提交成功(0)
push data[type=1, serial=MBCP00000011, len=1017] via MB FAILED, 剩余:1
RECV data from IOT, len=532
RECV data from IOT, len=532
push data[type=2, serial=MBCP00000012, len=1017] via MB SUCCESSED, 剩余:0
iot_status:0
RECV data from IOT, len=532
作业数据(serial:0000000000, 流水:006EA1B2C3D4E5202412161643210010,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
HTTP丢包率：1/9
data[type=512,serial=006EA1B2C3D4E5202412161644200012] 入待发送队列
push data[type=512, serial=MBCP00000013, len=413] via MB FAILED, 剩余:0
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_40, M_40, L_40
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_40, M_40, L_40
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_40, M_40, L_40
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_40, M_40, L_40
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_160, M_160, L_160
Total consumption of ink on startup：9_[V], [PRINT]S_0, M_0, L_0, [FLASH]S_160, M_160, L_160
iot_status:0
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
Total consumption of ink on startup：0_[K], [PRINT]S_400, M_400, L_400, [FLASH]S_280, M_280, L_280
Total consumption of ink on startup：1_[C], [PRINT]S_400, M_400, L_400, [FLASH]S_280, M_280, L_280
Total consumption of ink on startup：2_[M], [PRINT]S_400, M_400, L_400, [FLASH]S_280, M_280, L_280
Total consumption of ink on startup：3_[Y], [PRINT]S_400, M_400, L_400, [FLASH]S_280, M_280, L_280
Total consumption of ink on startup：8_[W], [PRINT]S_1600, M_1600, L_1600, [FLASH]S_1120, M_1120, L_1120
Total consumption of ink on startup：9_[V], [PRINT]S_1600, M_1600, L_1600, [FLASH]S_1120, M_1120, L_1120
HTTP丢包率：1/9
data[type=512,serial=006EA1B2C3D4E5202412161645210013] 入待发送队列
push data[type=512, serial=MBCP00000014, len=413] via MB FAILED, 剩余:0
Total consumption of ink on startup：0_[K], [PRINT]S_800, M_800, L_800, [FLASH]S_320, M_320, L_320
Total consumption of ink on startup：1_[C], [PRINT]S_800, M_800, L_800, [FLASH]S_320, M_320, L_320
Total consumption of ink on startup：2_[M], [PRINT]S_800, M_800, L_800, [FLASH]S_320, M_320, L_320
Total consumption of ink on startup：3_[Y], [PRINT]S_800, M_800, L_800, [FLASH]S_320, M_320, L_320
Total consumption of ink on startup：8_[W], [PRINT]S_3200, M_3200, L_3200, [FLASH]S_1280, M_1280, L_1280
Total consumption of ink on startup：9_[V], [PRINT]S_3200, M_3200, L_3200, [FLASH]S_1280, M_1280, L_1280
iot_status:0
RECV data from IOT, len=532
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=2,serial=006EA1B2C3D4E5202412161645510014] 入待发送队列
push data[type=2, serial=MBCP00000015, len=1015] via MB FAILED, 剩余:0
data[type=2, serial=006EA1B2C3D4E5202412161645510014] 重入待发送队列
RECV data from IOT, len=532
RECV data from IOT, len=532
push data[type=2, serial=MBCP00000016, len=1015] via MB SUCCESSED, 剩余:0
iot_status:0
RECV data from IOT, len=532
作业数据(serial:0000000000, 流水:006EA1B2C3D4E5202412161645510014,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
HTTP丢包率：1/10
data[type=512,serial=006EA1B2C3D4E5202412161646220015] 入待发送队列
push data[type=512, serial=MBCP00000017, len=398] via MB SUCCESSED, 剩余:0
iot_status:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202412161646220015,提交成功(0)
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
HTTP丢包率：1/11
data[type=512,serial=006EA1B2C3D4E5202412161647230016] 入待发送队列
push data[type=512, serial=MBCP00000018, len=413] via MB SUCCESSED, 剩余:0
iot_status:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202412161647230016,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
HTTP丢包率：1/12
data[type=512,serial=006EA1B2C3D4E5202412161648240017] 入待发送队列
push data[type=512, serial=MBCP00000019, len=415] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202412161648240017,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
HTTP丢包率：1/13
data[type=512,serial=006EA1B2C3D4E5202412161649250018] 入待发送队列
push data[type=512, serial=MBCP00000020, len=415] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202412161649250018,提交成功(0)
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
HTTP丢包率：1/14
data[type=512,serial=006EA1B2C3D4E5202412161650260019] 入待发送队列
push data[type=512, serial=MBCP00000021, len=415] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202412161650260019,提交成功(0)
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
HTTP丢包率：1/15
data[type=512,serial=006EA1B2C3D4E5202412161651270020] 入待发送队列
push data[type=512, serial=MBCP00000022, len=415] via MB SUCCESSED, 剩余:0
iot_status:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202412161651270020,提交成功(0)
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
HTTP丢包率：1/16
data[type=512,serial=006EA1B2C3D4E5202412161652280021] 入待发送队列
push data[type=512, serial=MBCP00000023, len=401] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202412161652280021,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
HTTP丢包率：1/17
data[type=512,serial=006EA1B2C3D4E5202412161653290022] 入待发送队列
push data[type=512, serial=MBCP00000024, len=413] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202412161653290022,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
HTTP丢包率：1/18
data[type=512,serial=006EA1B2C3D4E5202412161654300023] 入待发送队列
push data[type=512, serial=MBCP00000025, len=415] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202412161654300023,提交成功(0)
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
HTTP丢包率：1/19
data[type=512,serial=006EA1B2C3D4E5202412161655310024] 入待发送队列
push data[type=512, serial=MBCP00000026, len=415] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202412161655310024,提交成功(0)
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
HTTP丢包率：1/20
data[type=512,serial=006EA1B2C3D4E5202412161656320025] 入待发送队列
push data[type=512, serial=MBCP00000027, len=399] via MB SUCCESSED, 剩余:0
iot_status:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202412161656320025,提交成功(0)
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
HTTP丢包率：1/21
data[type=512,serial=006EA1B2C3D4E5202412161657330026] 入待发送队列
push data[type=512, serial=MBCP00000028, len=415] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202412161657330026,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
HTTP丢包率：1/22
data[type=512,serial=006EA1B2C3D4E5202412161737310027] 入待发送队列
push data[type=512, serial=MBCP00000029, len=415] via MB FAILED, 剩余:0
HTTP丢包率：1/22
data[type=512,serial=006EA1B2C3D4E5202412161742170028] 入待发送队列
push data[type=512, serial=MBCP00000030, len=415] via MB FAILED, 剩余:0
Total consumption of ink on startup：0_[K], [PRINT]S_800, M_800, L_800, [FLASH]S_360, M_360, L_360
Total consumption of ink on startup：1_[C], [PRINT]S_800, M_800, L_800, [FLASH]S_360, M_360, L_360
Total consumption of ink on startup：2_[M], [PRINT]S_800, M_800, L_800, [FLASH]S_360, M_360, L_360
Total consumption of ink on startup：3_[Y], [PRINT]S_800, M_800, L_800, [FLASH]S_360, M_360, L_360
Total consumption of ink on startup：8_[W], [PRINT]S_3200, M_3200, L_3200, [FLASH]S_1440, M_1440, L_1440
Total consumption of ink on startup：9_[V], [PRINT]S_3200, M_3200, L_3200, [FLASH]S_1440, M_1440, L_1440
iot_status:0
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
HTTP丢包率：1/22
data[type=512,serial=006EA1B2C3D4E5202412161743180029] 入待发送队列
push data[type=512, serial=MBCP00000031, len=415] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202412161743180029,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
HTTP丢包率：1/23
data[type=512,serial=006EA1B2C3D4E5202412161744190030] 入待发送队列
push data[type=512, serial=MBCP00000032, len=415] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202412161744190030,提交成功(0)
iot_ccid:CCID-123, imei:IMEI-123
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
CLOUD_PLATFORM线程退出
CloudServiceCore线程退出
云模块版本:2.1.0.0
DATA SUBCRIBER:[CLOUD_PLATFORM,]
iot_status:3
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:0
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
The mainboard is not initialized. 
The mainboard is not initialized. 
The mainboard is not initialized. 
The mainboard is not initialized. 
The mainboard is not initialized. 
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
iot_status:3
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=2,serial=FFFFFFFF202412161757210000] 入待发送队列
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=2,serial=FFFFFFFF202412161757400001] 入待发送队列
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
The mainboard is not initialized. 
The mainboard is not initialized. 
The mainboard is not initialized. 
Total consumption of ink on startup：0_[K], [PRINT]S_204040, M_1064, L_237552, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_204040, M_1064, L_237552, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_204948, M_1064, L_237552, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_204040, M_1064, L_237552, [FLASH]S_0, M_0, L_0
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=2,serial=FFFFFFFF202412161758130002] 入待发送队列
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=2,serial=FFFFFFFF202412161802050003] 入待发送队列
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
CLOUD_PLATFORM线程退出
The mainboard is not initialized. 
CloudServiceCore线程退出
云模块版本:2.1.0.0
DATA SUBCRIBER:[CLOUD_PLATFORM,]
iot_status:3
iot_status:3
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
iot_status:3
The mainboard is not initialized. 
The mainboard is not initialized. 
iot_status:3
CLOUD_PLATFORM线程退出
The mainboard is not initialized. 
CloudServiceCore线程退出
