


**Large Format Printer setup in Maintop Software.**




**1.Open your Maintop Software and access Printer Setup via File Menu**



**2. On the pop-up window click on Install**




**3. Click on Custom**



**4. From the Utility disc locate the Driver(.inf) and click Open. Link given below**


\FastCOLOUR Printer\Maintop Driver for FastCOLOUR DX5,DX7 Single Head\MT-ECO Driver for Solvent and ECO-Solvent Ink

If you are no longer in possession of the utility disc you can access it from am.co.za/utility/disc




**5. Printer will then appear under “Installed Printers” Click OK to finish** 


**Printing from Maintop Software**



**1.From your toolbar click on the Print Icon** 




**2.Click on Properties** 

1.Change resolution to 720\*2160dpi

2.Under Print Media select the required number of Passes. Please note the selection has to correspond to the **number of passes on the Pass option**.

**3.Click OK to save the desired settings**



**4.Click OK to print**