**Those Are NOT Normal Batteries**

|  |  |  |  |
| --- | --- | --- | --- |
| ReservedBattery | ReservedBattery | Live | Live |

**When you see ERR 40**

1. Keep Machine On (very important)
2. Remove the batteries in “Live” Position
3. Put Batteries in “Reserved” potion to “Live” Position
4. Reboot machine

Remember buy another two batteries to Reserve for next battery change.

* Size: AA
* Voltage: 3.6V
* Type: Lithium

Contact AM.CO.ZA Support if you failed to change battery or machine position shifted during battery change.

WhatsApp 060 600 6000