en-US

# Edit IP Addresses of Multiple Cameras

You can batch modify the IP addresses of multiple cameras under the same interface.

1. Select a network interface.
2. Select the cameras to be modified.
   Note:

   You can select up to 20 cameras.

3. Click Modify IP to open the Batch Modify IP window.
   Figure 1 Batch Modify IP Addresses
4. Select Static IP, DHCP, or LLA as the IP type.
   Note:

   - For setting the IP type as Static IP, you can set the start IP address, subnet mask, and default gateway.

   - For batch modifying static IP, you only need to configure the start IP address. The last decimal of the next IP address will be plus 1, and so forth (example: 192.168.1.1, 192.168.1.2, 192.168.1.3...).

5. Click OK to save the settings.
   Note:

   If the modified IP address conflicts with another device's IP address in the same local subnet, a prompt will pop up to remind you that IP conflict occurs. Change the IP address in this situation.