en-US

# Other Features

Configure the following parameters according to your need.

Binning Selector

  Selects which binning engine is controlled by the BinningHorizontal and BinningVertical features.

Binning Horizontal/Vertical

  Number of horizontal/vertical pixels to combine together.

Decimation Horizontal/Vertical

  Horizontal/vertical sub-sampling of the image.

Shading Selector

  Selects the mode of shading correction.

Activate Shading

  Activates the selected shading set.

NUC Enable

  Enable the FPNC and PRNUC Control

PRNUC User Enable

  Enable PRNUC user table

Event Selector

  Selects which Event to signal at the host application.

Event Notification

  This enumeration sets the type of a notification that will be sent to the host application for the selected event.