en-US

# Add Remote Camera

You can add GigE Vision camera NOT in the same local subnet with the client software to the device list.

1. Right-click the network interface card (for example, Local Area Connection in the following picture) to open the right-click menu.
   Figure 1 Right-click Menu
2. Click Add Remote Camera to open the Add Remote Camera window.
   Figure 2 Add Remote Camera
3. Enter the camera IP address and then click OK to add the camera.