en-US

# Import/Export Features of a Single Device

You can export the feature configurations of the selected device as an MFS or HCF file to the local PC, and import the file from the local PC to the selected devices to fast configure all its features without the inconvenience of configuring its features one by one.

Connect the camera or frame grabber to the Software and make sure its image data acquisition has been stopped.

To export features of a selected camera, you only need to click . If you need to import features of a single camera, perform the following steps.

Note:

- The read-only feature cannot be exported.

- The exported information doesn't contain camera IP address, MAC address, serial No., and user ID.

1. Click and then select a file from the local PC.
   Note:

   - For cameras, select an MFS file; for frame grabbers, select an HCF file.

   - Only when the model of the source camera or frame grabber is same with that of the target camera or frame grabber can the file be imported.

2. Click Import to import the feature configurations.