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逻辑版本提测说明
  




	作者
	庞高峰

	硬件版本
	HEB-F_01-JB2X24_02X24_02 V1.1.0.*（1.43） 

	逻辑版本
	HBL_1.43_I1600_4H_V12.1.1.0.1803_20241101

	git SHA
	SHA-1: 62697c54037499c12e4cce9d6c3ad66259ce797d







[bookmark: _Toc140776621]版本需求描述
[bookmark: _Toc93398214]1、1.43板卡支持新通信协议。
[bookmark: _Toc140776622]功能描述
逻辑修改支持兼容新协议，参考1.24。
[bookmark: _Toc140776623]。时序分析报告
时序无违例，时序报告如下：
 
[image: ]

[bookmark: _Toc140776624]自测报告
通讯测试
测试环境：桌面环境。
[image: ]
测试方法：KT设置新、旧协议后，分别测试升级、读写寄存器功能。
测试结果：新、旧协议升级功能正常，读写寄存器功能正常。
[image: ]
[bookmark: _Toc140776630]注意事项
测试重点内容： 
1、 [bookmark: _GoBack]不同主板连接喷车板通讯测试。
2、 新、旧协议通常测试。


image2.png
23 slp_rx_otrlv £ HEB_T1600_phy. area. [x] - Report
Report Navigation Device Package ReportLevel Errors Paths Coverage Setup Slack Hold Slack Time

Timing summary 1 eagle 20 BGA256X Detai 0 1413340 9077% 0624ns  0.006ns  2024-11-01 20:17:07
~ Timing constraints

dlock: link_ctrl/RBC_PLL inst/pll.

clock:

clock: u_misc_ctrl/pl Timing group statistics.

clock: u_misc_ctr/pl v Timing group statistics:

clock: u_misc_ctr/pl ' v Clock constraints:

Setinput delay: 10ns max, and.. Clock Name Min Period Max Freg Skew  Fanout
u_misc_ctrl/pll_inst/pll_inst.clkc[0] (SO.0MHz) 18.587ns saumz 0.612ns 3264
u_misc_ctrl/pll_inst/pll_inst.clkc[4] (40.0MHz) 13.511ns TaMHz 0.524ns sae
link_ctrl/RBC_PLL inst/pll_inst.clkc[0] (40.0MAz) 14.080ns Timz 0.128ns s
link_ctrl/RBC_PLL inst/pll_inst.clkc[1] (80.0MAz) 11.876ns samnz 0.128ns E
u_misc_ctrl/pll_inst/pll_inst.clkc[3] (80.0MHz) 3.874ns 258Mz 0.571ns 26

Minimum input arrival time before clock 2.507ns
Maximum output required time after clock no constraint path
Maximum combinational path delay no constraint pach
v Exceptions:
v Check Type: MAX
Path Num Constraint
759 set_false_path ~from [ get_clocks {u_misc_ctrl/pll_inst/.
653 set_false_path ~from [ get_clocks {u_misc_ctrl/pll inst/.
v Check Type: MIN
Path Num Constraint
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